BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1038
Forward CLI/COL

This command is used to state, whether the received calling/connected number (CLI/COL) is to be forwarded in case of transit/gateway, or external diverted call.

##### Valid data

Value = |  | 0 |  | Forward for transit/gateway calls, except to public net (Intial value) |
|  | 1 |  | Forward for transit/gateway calls |
|  | 2 |  | Forward for transit/gateway calls and external diverted calls |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005