BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2004
National key (Hold)

Text to be printed on a printer or shown on a display can be defined via DIALOG 2753, DIALOG 2754, DIALOG 2662 and DIALOG 2663.

The following survey shows both non-programmable and programmable keys.

The table shows only the keys for system instruments. The corresponding keys on operator instruments have the same values.

KEY | DIALOG 2662 | DIALOG 2753
ASCII | Character | ASCII | Character
0-9 | 30-39 | 0-9 | 30-39 | 0-9
* | 2A | * | 2A | *
# | 23 | # | 23 | #
A-Z | 41-5A | A-Z | 41-5A | A-Z
INQUIRY | **) | (Command 2003) | **) | (Command 2006)
HOLD | **) | (Command 2004) | 2E | .
READ & | **) | (Command 2005) | 20 | Space
TRANSFER | **) | (Command 2006) | 3A | :
SAVE | 20 | Space | 27 | ‘
CONF | 2E | . | -- |
LINE 1 | 2F | / | **) | (Command 2004)
LINE 2 | 27 | ‘ | **) | (Command 2005)
DIVERSION | 3F | ? | **) | (Command 2003)
MUTE | -- |  | 2D | -
PICKUP | -- |  | 2F | /
MENU *) | 2B | + | 2B | +
INFO *) | 2D | + | 2C | ,
MESSAGE *) | 2D | & | 26 | &
PROG *) | -- |  | 3D | =
F1 *) | 21 | ! | 21 | !
F2 *) | 3A | : | 3F | ?
F3 *) | 2C | , | 28 | (
F4 *) | 26 | & | 29 | )

**) By means of commands 2003 National key (Inquiry)-2006 National key (Transfer), it is possible to select the character to be shown on depression of a key. |  |

*) These keys can be used for input of text, but not for all facilities. |  |

The table below lists the characters that are obtained for different values of the data in the command.

ASCII | Function
20-7D | Standard US ASCII
D1-FF | Special characters

STANDARD US ASCII, 20-7D

| 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | A | B | C | D | E | F
20 |  | ! | “ | # | $ | %% | & | ‘ | ( | ) | * | + | , | - | . | /
30 | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | : | ; | < | = | > | ?
40 | @@ | A | B | C | D | E | F | G | H | I | J | K | L | M | N | O
50 | P | Q | R | S | T | U | V | W | X | Y | Z | [ | \ | ] | ^ | _
60 | ‘ | a | b | c | d | e | f | g | h | i | j | k | ] | m | n | o
70 | p | q | r | s | t | u | v | w | x | y | z | { | | | } | -> | <-

SPECIAL CHARACTERS, D1-FF

Values for which no character is given are not defined.

D1 = † |  |

D2 = |  |

D3 = Ž |  |

D4 = š |  |

D9 = › |  |

DA = ‘ |  |

DB = Empty square |  |

DC = “ |  |

DF = ø |  |

E1 = “ |  |

ED = ˝ |  |

EE = ¤ |  |

EF = (tm) |  |

F5 = |  |

FC = ‘ |  |

FF = þ |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005