BusinessPhone Communication Platform 7.0
Commands > Commands 5000...5999

## 5411
Create call number for alternative paging

ASB 150 permits connection of external equipment for paging via radio or a magnetic loop. Connection is achieved via a trunk (external line) board that has been reserved for this purpose.

This command is used to create a function for alternative paging. The stated directory number must be free and must not conflict with any existing directory number; it is used to set up paging. Alternative paging means that the pager himself/herself can control the paging receiver by stating a mode digit, sending a message or supplying a spoken message.

Command 5410 Create call number for standard paging is used to create a function for “standard” paging and command 5412 Create answer number for meet-me is used to create a function for answer in accordance with the meet-me principle.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005