BusinessPhone Communication Platform 7.0
Commands > Commands 9000...9999

## 9004
Active time for ’CBack on busy’ superPBX

This command specifies the time during which a network Call Back on Busy mission is active in the supervised PBX.

If this timer expires the Call Back mission in the supervised PBX is deleted and the Call Back has failed.

This timer can be programmed to values in steps of 5 minutes.

This timer must be programmed to the same value in every PBX which makes use of network Call Back.

The value of this timer must be at least 5 minutes above the corresponding one in the initiating PBX (command 9002 Active time for ’CBack on busy’ initPBX).

Values: 0010 (= 10 minutes) to 0900 (= 9 hours) using the format ‘hhmm’ |  |

Initial Value: 0205 (= 2 hours 5 minutes) |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005