BusinessPhone Communication Platform 7.0
BMS Script Programmers Reference

## Script language, BMS Objects reference

### BMS Managed Objects (System data)

2001 |  | Ring signal scheme
2001
Value | GUI
"0" | Standard (CCITT)
"1" | Sweden
"2" | Denmark, Norway
"3" | Italy
"4" | Spain Option 1
"5" | Spain Option 2
"6" | United Kingdom
"7" | Malaysia
"8" | Undefined
"9" | Undefined

2003 |  | National key (Inquiry)

Value: 20 (hex) – 7F (hex),D1 (hex) – FF (hex)

2004 |  | National key (Hold)

Value: 20 (hex) – 7F (hex),D1 (hex) – FF (hex)

2005 |  | National key (Read&)

Value: 20 (hex) – 7F (hex),D1 (hex) – FF (hex)

2006 |  | National key (Transfer)

Value: 20 (hex) – 7F (hex),D1 (hex) – FF (hex)

2007 |  | Rotary dial type

2008 |  | Verification tone on call back

Value: "true"/"false" Default: "true"

2011 |  | PCM-channels reserved for external lines

Value range: "0" – "60"

2023 |  | External voice mail directory number

Value: max. 8 digits (0-9)

2025 |  | Nominal impedance for analogue extensions

2026 |  | Attenuation for DTMF-signalling

2027 |  | Length of inactivity tone

Value range: "1"-"255" seconds

2028 |  | Ringtime for internal calls

Value range: "1"-"255" seconds

2029 |  | Repetitive call-waiting tone

Value: "true"/"false"

2030 |  | Disconnection tone for digital extensions

Value: "true"/"false"

2032 |  | Side tone masking rating
2032
Value | GUI
"0" | 8 dB (-17 dBr max)
"1" | 9 dB (-18 dBr)
"2" | 10 dB (-19 dBr)
"3" | 11 dB (-20 dBr)
"4" | 12 dB (-21 dBr)
"5" | 13 dB (-22 dBr)
"6" | 14 dB (-23 dBr)
"7" | 15 dB (-24 dBr)
"8" | 16 dB (-25 dBr)
"9" | 17 dB (-26 dBr)
"10" | 18 dB (-27 dBr)
"11" | 19 dB (-28 dBr)
"12" | 20 dB (-29 dBr)
"13" | 21 dB (-30 dBr)
"14" | 22 dB (-31 dBr)
"15" | 23 dB (-32 dBr min)

2033 |  | Sending Loudness Rating

2036 |  | Call pickup of reminder/call back allowed

Value: "true"/"false"

2039 |  | Music on hold after transfer

Value: "true"/"false"

2056 |  | Shut down reroute position

Value: max. 4 digits (0-9,*,#)

2080 |  | Free second access

Value: "true"/"false"

2082 |  | Transfer via hookon

Value: "true"/"false"

2060 |  | Consolidation time from alarm to OK

Value range: "0"-"255"

2061 |  | First priority link for synchronisation

Value: Trunk card, ICCU card, MFU card. The submitted value consists of 5 digits. The first two stand for the card position (01 for card 1,…), the last three values are set to "000".

2062 |  | Second priority link for synchronisation

Value: Trunk card, ICCU card, MFU card. The submitted value consists of 5 digits. The first two stand for the card position (01 for card 1,…), the last three values are set to "000".

2063 |  | Third priority link for synchronisation

Value: Trunk card, ICCU card, MFU card. The submitted value consists of 5 digits. The first two stand for card position (01 for card 1,…) the last three values are set to "000".

2064 |  | Fourth priority link for synchronisation

Value: Trunk card, ICCU card, MFU card. The submitted value consists of 5 digits. The first two stand for the card position (01 for card 1,…) the last three values are set to "000".

2065 |  | Fifth priority link for synchronisation

2090 |  | VPN Service from PSTN

Value: "true"/"false"

2091 |  | Predigits sent to PSTN-VPN

Value range: 8 digits (0-9)

2092 |  | Trunk route selected as PSTN-VPN call

Value: trunk route (directory number)

2093 |  | Conversation recording tone

Value: "true"/"false"

2094 |  | GAP Version

2101 |  | Recall on parking

Value range: "0"-"255" seconds; "0" = no recall

2104 |  | Recall on individual parking

Value range: "0"-"255" seconds; "0" = no diversion

2105 |  | Minimum release signal

Value range: "10"-"99" in steps of 10ms

2106 |  | Minimum register signal

Value range: "4"-"99" in steps of 10ms

2108 |  | MFE time 1

Value range: "5"-"20" seconds

2109 |  | MFE time 2

Value range: "5"-"20" seconds

2110 |  | Delay voice announcement

Value range: "0"-"30" seconds

2111 |  | Alerting timeout for cordless

Value range: "5"-"30" seconds

##### Attribute (24xx)

Value: 6 digits: xxxxxx (each digit has a value from 0-9)

This attribute consist of 2401, 2402, 2403, 2406, 2407, 2408 attributes. Each attribute corresponds to one command.

2401 |  | Digit for camp-on

Value range: "0"-"9", blank

2402 |  | Digit for Call back

Value range: "0"-"9", blank

2403 |  | Digit for Call pick up

Value range: "0"-"9", blank

2406 |  | Digit for Executive intrusion

Value range: "0"-"9", blank

2407 |  | Digit for Radio paging

Value range: "0"-"9", blank

2408 |  | Digit for Message

Value range: "0"-"9", blank

7506 |  | High traffic limit timer

Value Range: "0" – "250"

7507 |  | Max traffic limit timer

Value Range: "0" – "255"

2070 |  | Keypad characters

##### Attribute (2070_0) Keypad characters button 0

Value: all printable characters, Length: 30

##### Attribute (2070_1) Keypad characters button 1

Value: all printable characters, Length: 30

##### Attribute (2070_2) Keypad characters button 2

Value: all printable characters, Length: 30

##### Attribute (2070_3) Keypad characters button 3

Value: all printable characters, Length: 30

##### Attribute (2070_4) Keypad characters button 4

Value: all printable characters, Length: 30

##### Attribute (2070_5) Keypad characters button 5

Value: all printable characters, Length: 30

##### Attribute (2070_6) Keypad characters button 6

Value: all printable characters, Length: 30

##### Attribute (2070_7) Keypad characters button 7

Value: all printable characters, Length: 30

##### Attribute (2070_8) Keypad characters button 8

Value: all printable characters, Length: 30

##### Attribute (2070_9) Keypad characters button 9

Value: all printable characters, Length: 30

##### Attribute (2070_10) Keypad characters button *

Value: all printable characters, Length: 30

#### MO(AccCode)

##### Attribute (2114_<X>) Valid Account Codes

Whereas X = 0..999

Value: 1 to 10 digits (decimal)

#### MO(AutoRedial)

2271 |  | Number of Automatic Redial Requests

Value range: 0-99 (decimal)

2272 |  | Trunks Available for Automatic Redial

Value: BC 8, BC 9, BC 10/1, BC 10/2

Initial value = BC 8

2273 |  | Automatic Redial Trunk Access Retries

Value range: 0-3 (decimal)

2274 |  | Automatic Redial Answer Supervision Time

Value: 0 to 4 digits

##### Attribute (2275_<X>) First central answering position

Whereas X = 1..10

Value: 'blank', 1-8 digit number

#### MO(Tones)

See additional documents.

2610 |  | Number of DTMF tones
2610
Value | GUI
"0" | 12
"1" | 16

2611 |  | Level

Value: "-64.0"-+"3.0" dBm0 in steps of 0.5 dBm0

2612 |  | Level difference

Value: "1"-"3" dBm0 in steps of 0.5 dBm0

2613 |  | Signal time

Value: "0"-"32768"

2614 |  | Pause time

Value: "0"-"32768" ToneFragment

##### Attribute (2601_XX )

Whereas XX = 1 … 19

Value Range: "-64.0" – "3.0" dB

(Step: 0.5 dB)

##### Attribute (2602_XX)

Whereas XX = 1 … 19

Value Range: "300" – "3400" Hz

##### Attribute (2603_XX)

Whereas XX = 1 … 19

Value Range: "-64.0" – "3.0" dB

(Step: 0.5 dB)

##### Attribute (2604_XX)

Whereas XX = 1 … 19

Value: 5 digits (Hz)

##### Fixed Tones

It is not recommended to set values for fixed tones MO directly. The fixed tone values are changed through Tones MOs described later on in this chapter.

#### Tones 2620 - 2650

- Tone MO´s list:

##### MO(Tone_2620)

MO(Tone_2621)

MO(Tone_2622)

MO(Tone_2623)

MO(Tone_2624)

MO(Tone_2625)

MO(Tone_2626)

MO(Tone_2627)

MO(Tone_2628)

MO(Tone_2629)

MO(Tone_2630)

MO(Tone_2631)

MO(Tone_2632)

MO(Tone_2633)

MO(Tone_2634)

MO(Tone_2635)

MO(Tone_2636)

MO(Tone_2637)

MO(Tone_2638)

MO(Tone_2639)

MO(Tone_2640)

MO(Tone_2641)

MO(Tone_2642)

MO(Tone_2643)

MO(Tone_2644)

MO(Tone_2645)

MO(Tone_2646)

MO(Tone_2647)

MO(Tone_2648)

MO(Tone_2649)

MO(Tone_2650)

Each listed MO has the following attributes:

##### Attribute (FixedTone)

Value: digit (0..4)

##### Attribute (Repetition)

Value Range: "0" – "3"

##### Attribute (TFint_NN)

Whereas NN = 1 to 4

Value Range: "0" – "19" (15)

##### Attribute (TFext_NN)

Whereas NN = 1 to 4

Value Range: "0" – "19" (15)

##### Attribute (SigTime_NN)

Whereas NN = 1 to 4

Value Range: "0" – "16000" s (no value means continuous)

##### Attribute (PauseTime_NN)

Whereas NN = 1 to 4

Value Range: "0" – "16000" s (no value means continuous)

#### MO(IncExt)

2222 |  | Number Serial Range

##### Attribute (min_<XX>)

Whereas XX = 0 to 9

Value: exactly 2 digits (0-9) or empty

##### Attribute (max_<XX>)

Whereas XX = 0 to 9

Value: exactly 2 digits (0-9) or leave the value empty

#### MO(PubDir)

2220 |  | Public number

##### Attribute (2220_NN)

Whereas NN = 0 to 31

Value: max. 16 digits (0-9)

2224 |  | Type

##### Attribute (2224_NN)

Whereas NN = 0 to 31

2224_x, whereas X = 0 to 31
Value | GUI
"0" | unknown
"1" | international
"2" | national
"3" | network-specific
"4" | subscriber

2236 |  | Own country code

Value: max. 4 digits (0-9,*,#)

2237 |  | Own area code

Value: max. 4 digits (0-9,*,#)

2023) External voice mail directory number (R12) |  |

Value: max. 8 digits (0-9)

#### MO(Transmission0)

2710 |  | Transmission Group 0

##### Attribute (<XY>R) The relative receiving level

Whereas X = 1 to 9, Y = 0 to 4

Value range: of -12 dBr and +6 dBr in steps of 0.1 dB

##### Attribute (<NN>S) The relative sending level

Whereas X = 1 to 9, Y = 0 to 4

Value range: -12 dBr and +6 dBr in steps of 0.1 dB

2731 |  | Transmission level

##### Attribute (2731_NN)

Whereas NN = 0 to 3

Value range: -12dB – 6dB (Step 0.1 dB)

#### MO(Transmission17)

2720 |  | The transmission matrix

##### Attribute (<XY>R) The relative receiving level

Whereas X = 1 to 9, Y = 0 to 7

Value range: of -12 dBr and +6 dBr in steps of 0.1 dB

##### Attribute (<NN>S) relative sending level

Whereas X = 1 to 9, Y = 0 to 4

Value range: of -12 dBr and +6 dBr in steps of 0.1 dB

#### MO(INT)

2260 |  | DDI/CN number translation

##### Attribute (2261<X>_<YY>) Internal Directory Number

Whereas X= a, b YY=0..199

Value: max. 4 digits (0-9)

##### Attribute (2262_<XX>) DDI number 1

Whereas X = 0..199

Value: max. 8 digits (0-9)

##### Attribute (2263_<XX>) DDI number 2

Whereas X = 0..199

Value: max. 8 digits (0-9)

2263 |  | Type of individual number translation

Value range: 0-4

#### MO(PDNT)

2240 |  | Public Destination Numbers

2241 |  | Predigits

Value: max. 5 digits (0-9)

Initial value =""

2242 |  | The leading digits of a destination number

##### Attribute (2242_<X>)

Whereas X = 0..999

Value: max. 10 digits (0-9)

Initial value =""

2243 |  | The number of the group

##### Attribute (2243_<X>)

Whereas X = 0..999

Value range: "0"-"249"

Initial value =""

#### MO(DNCT)

2250 |  | Destination Number Cross Reference Table

##### Attribute (2251_<X>) Predigits

Whereas X = 1..4

Value: max. 4 digits (0-9)

Initial value =""

##### Attribute (2252_<X>_<Y> ) The leading digits of a destination number

Whereas X = 1..4, Y = 0..199

##### Attribute (2255_<X>) The number of the group

Whereas X = 0..199

Value range: "249"-"0"

Initial value =""

max. 50 groups

#### MO(PSTN)

2221 |  | PSTN-operator call numbers

##### Attribute (2221_<X>)

Whereas X = 0 to 10

Value: max. 3 digits (0-9)

#### MO(TCD)

2201 |  | Open number interval

##### Attribute (2201a_<XX>)

Whereas XX = 0 to 99

Value: max. 10 digits (0-9,*,#)

##### Attribute (2201b_<XX>)

Whereas XX = 0 to 99

2202 |  |

to

2209 |  | Open for TCD category 8

##### Attribute (2202_<XX>)

Whereas XX = 0 to 99

Value: 8 digits (0=closed,1=open)

Note

The bit position (0-7) corresponds to command (2202-2209).

2088 |  | TCD for suffix dialling when authority code active (day-switched)

2089 |  | TCD for suffix dialling when authority code active (night-switched)

#### MO(Traffic)

2301 |  |

to

2315 |  | Traffic group discrimination 15

##### Attribute (23<XX>_<YY>)

Whereas X = 1 to 15, YY = 1,2

XX==1 Value=7 digits (0-1)

XX==2 Value=8 digits (0-1)

2340 |  | Traffic check at conference

Value range: "0"-"9"

2341 |  | Traffic check at operator conference

Value range: "0"-"9"

2342 |  | Traffic check at call pick-up

Value range: "0"-"9"

2343 |  | Traffic check at break-in

Value range: "0"-"9"

#### MO(RSU)

7801 |  | RSU-group reservation

##### Attribute (7801_8_110)

Value range: {0,1,2}

##### Attribute (7801_8_116)

Value range: {0,1,2}

#### MO(TenantDef)

6801 |  | Tenant name

##### Attribute (6801_<XX>)

Whereas X = 1..15

Value: 40 characters

6802 |  | Tenant password

##### Attribute (6802_<XX>)

Whereas X = 1..15

Value: 10 digits (0-9)

6803 |  | Tenant-Route

##### Attribute (6803_<XX>)

Whereas X = 1..15

Value: 4 digits (0-9,*,#); trunk route directory number

#### MO(Password)

No commands/attributes

#### MO(ExDays)

#### MO(Clock)

No commands/attributes

#### MO(Test Call)

5414 |  | Test call numbers

##### Attribute (TestCall_<XX>)

Whereas X = 0 to 4

Value: 4 digits (0-9,*,#); directory number

#### MO(System Access)

5621 |  | Define System access

##### Attribute (SystemAccess_0)

Value: 4 digits (0-9,*,#); directory number

#### MO(IPUMan)

##### Attribute (2163_<X> ) Signaling protocol

Whereas X = 0 to <Individual count>

Value range: 0-255

Signaling protocol
Value | Description
"0" | None
"1-100" | Reserved
"101" | ASB150 02 IP Gateway
"102-255" | Reserved

##### Attribute (2164<X>_<Y>) Network IP address

Whereas X = a,b,c,d

Whereas a,b,c,d built IP address

Value range: 0-255

##### Attribute (2164d_<Y>) Network IP address port number

Whereas Y = 1 to 1000

Value range: 0-65535

##### Attribute (2169<X>_<Y>) Optimal media packet size table

Whereas X = a,b and Y = 1 to 16

Value range: 10-65535

Valid values/steps depend on the protocol (see Help). Temporary used attributes are 2169b_1 till 2169b_5.

#### IPU (<Card<X>_<Y>)

X is the card position number, and Y is the individual number.

2151 |  | Preferred start-up protocol

Value range: 0-2

Preferred start-up protocol
Value | Protocol
"0" | NONE
"1" | BOOTP
"2" | DHCP

##### Attribute (2152_<X>) IP address (own)

Whereas X is index with value 1,2,3, or 4

Value range: 0-255

Default: 0

##### Attribute (2153_<X>) Gateway IP address

Whereas X is index with value 1,2,3, or 4

Value range: 0-255

Default: 0

##### Attribute (2154_<X>) Subnet mask

Whereas X is index with value 1,2,3, or 4

Value range: 0-255

Default: 0

2157 |  | First RTP-port number

Value range: 0 - 65535

2158 |  | Amount of RTP-sessions

Value range: 0 – 65535

Default value: 60

2159 |  | MAC address (read only)

Value: valid MAC address

2160 |  | Network connection (read only)

Value range: 0-2

Network connection
Value | Connection
"0" | undefined (no connection established)
"1" | 10 BaseT
"2" | 100 BaseT

##### Attribute (2161_<X>) Application,

Whereas X = 1-16

Value range: 2-255

Application
Value | Description
0 | No application (i.e. the port is not used)
1 | I/O port 1 (e.g. forVCom, etc.)
2 | I/O port 2 (e.g. forVCom, etc.)
3 | I/O port 3 (e.g. forVCom, etc.)
4 | I/O port 4 (e.g. forVCom, etc.)
5-100 | Spare
101 | ASB 150 02 IP gateway
102-255 | Reserved

##### Attribute (2162_<X>) Port number,

Whereas X = 1-16

Value range: 0 – 65535

2171 |  | Gatekeeper activated?

Value: "true", "false"

2172 |  | Gatekeeper identifier

Value: 0-35 characters

##### Attribute (2176_<X>) Gatekeeper zone definition

Whereas X = 1 to 48

Value range: 0-255

2178 |  | GK NGK heart beat time interval

Value range: 1-8 digit number

Default: blank

##### Attribute (2181_<X> ) Gatekeeper IP-address

Whereas X = 1 to 4

Value range: 0-255

#### MO(X251)

1980 |  | Packet Mode Communication Link parameters

##### Attribute (1980_LINKNO_<XX>)

Whereas XX = 1 to 32

Value range: "1"-"32"

##### Attribute (1980_AIFNO_<XX>)

Whereas XX = 1 to 32

Value range: 0-(6)14

##### Attribute (1980_BIFNO_<XX>)

Whereas XX = 1 to 32

Value range: 0-(6)14

##### Attribute (1980_ATEI_<XX>)

Whereas XX = 1 to 32

Value range: 0-63

##### Attribute (1980_BTEI_<XX>)

Whereas XX = 1 to 32

Value range: 0-63

##### Attribute (1980_CURR_CARDNO_<XX>)

Whereas XX = 1 to 3

Value: 0-32

##### Attribute (1980_PREV_CARDNO_<XX>)

Whereas XX = 1 to 3

Value: 0-32

##### Attribute (1980_CURR_CARDNO)

Value: 0-32

##### Attribute (1980_PREV_CARDNO)

Value: 0-32

#### MO(X252)

1980 |  | Packet Mode Communication Link parameters

##### Attribute (1980_LINKNO_<XX>)

Whereas XX = 1 to 32

Value range: "1"-"32"

##### Attribute (1980_AIFNO_<XX>)

Whereas XX = 1 to 32

Value range: 0-(6)14

##### Attribute (1980_BIFNO_<XX>)

Whereas XX = 1 to 32

Value range: 0-(6)14

##### Attribute (1980_ATEI_<XX>)

Whereas XX = 1 to 32

Value range: 0-63

##### Attribute (1980_BTEI_<XX>)

Whereas XX = 1 to 32

Value range: 0-63

##### Attribute (1980_CURR_CARDNO_<XX>)

Whereas XX = 1 to 3

Value: 0-32

##### Attribute (1980_PREV_CARDNO_<XX>)

Whereas XX = 1 to 3

Value: 0-32

##### Attribute (1980_CURR_CARDNO)

Value: 0-32

##### Attribute (1980_PREV_CARDNO)

Value: 0-32

#### MO(X253)

1980 |  | Packet Mode Communication Link parameters

##### Attribute (1980_LINKNO_<XX>)

Whereas XX = 1 to 32

Value range: "1"-"32"

##### Attribute (1980_AIFNO_<XX>)

Whereas XX = 1 to 32

Value range: 0-(6)14

Attribute (1980_BIFNO_<XX>)

Whereas XX = 1 to 32

Value range: 0-(6)14

##### Attribute (1980_ATEI_<XX>)

Whereas XX = 1 to 32

Value range: 0-63

##### Attribute (1980_BTEI_<XX>)

Whereas XX = 1 to 32

Value range: 0-63

##### Attribute (1980_CURR_CARDNO_<XX>)

Whereas XX = 1 to 3

Value: 0-32

##### Attribute (1980_PREV_CARDNO_<XX>)

Whereas XX = 1 to 3

Value: 0-32

##### Attribute (1980_CURR_CARDNO)

Value: 0-32

##### Attribute (1980_PREV_CARDNO)

Value: 0-32

#### MO(Maintenance)

No commands/attributes

#### MO(SW)

No commands/attributes

#### MO(DirectoryMO)

No commands/attributes

#### MO(ShortNumberMgr)

##### Attribute (ShortNumberSeries-<XX>)

Whereas XX = 1 to 15

Value: 4 digits (0-9,*,#); directory number

#### MO(ShortNumberSeries-<XX>)

Whereas XX = 1 to 15

##### Attribute (Dirno)

Value: 4 digits (0-9,*,#); directory number

2801 |  |

to

2816 |  | Abbreviated number open for tenant 15

Value: 15 digits {0=Close,1=Open}

2501 |  | Programming of abbreviated numbers

##### Attribute (2501_<XX>)

Whereas XX = 0 to 999

Value range: 23 digits (0-9,*,#)

2502 |  |

to

2505 |  | Abbreviated number category 3

##### Attribute (2502_<XX>)

Whereas XX = 0 to 999

Value: 4 digits {0=Close,1=Open}

##### Attribute (Dirname_<XX>)

Whereas XX = 0 to 999

Value: 35 characters

#### MO(FictiveNumberMgr)

##### Attribute (FictiveNumberSeries-<XX>)

Whereas XX = 1 to 15

Value: 4 digits (0-9,*,#); directory number

#### MO(FictiveNumberSeries-<XX>)

Whereas XX = 1 to 15 Attribute (Dirno)

Value: 4 digits (0-9,*,#); directory number

2831 |  |

to

2836 |  | Fictive number open for tenant 5

Value: 15 digits {0=Close,1=Open}

2531 |  | Assigned number

##### Attribute (2531_<XX>)

Whereas XX = 0 to 999

Value range: 23 digits (0-9,*,#)

2502 |  |

to

2505 |  | Abbreviated number category 3

##### Attribute (2502_<XX>)

Whereas XX = 0 to 999

Value: 4 digits {0=Close,1=Open}

##### Attribute (Dirname_<XX>)

Whereas XX = 0 to 999

Value: 35 characters

### BMS Managed Objects (ExtensionMgrMO)

No commands/attributes

#### ExtensionMO(<variable name>)

0101 |  | Facility COS

Value Range: 0 – 15

0102 |  | Traffic group

Value Range: 0 – 15

0103 |  | TCD-day COS

Value Range: 0 – 8

0104 |  | TCD-night COS

Value Range: 0 – 8

0105 |  | Common abbreviated number COS

Value Range: 0 – 3

0106 |  | Call back allowed?

Value: "true"/"false"

0107 |  | Break-in allowed?

Value: "true"/"false"

0108 |  | Camp-on allowed?

Value: "true"/"false"

0109 |  | Diversion active?

Value: "true"/"false"

0110 |  | Diversion on no reply at internal calls?

Value: "true"/"false"

0111 |  | Diversion on busy at internal calls ?

Value: "true"/"false"

0112 |  | Destination of fixed diversion

Value: 4 digits (0-9,*,#); directory number

0113 |  | Follow me

Value: 4 digits (0-9,*,#); directory number

0114 |  | Ringing line 1
0114
GUI | Value
No ringing | 0
Ringing (default) | 1
Ringing after 10s delay | 2
Only first ringing period- suppressed | 3
Only first ringing period- suppressed after 10s delay | 4
Ringing | 5

0115 |  | Ringing line 2
0115
GUI | Value
No ringing | 0
Ringing (default) | 1
Ringing after 10s delay | 2
Only first ringing period- suppressed | 3
Only first ringing period- suppressed after 10s delay | 4
Ringing | 5

0116 |  | Hot line destination

Value: 4 digits (0-9,*,#); directory number

0117 |  | Authority code?

Value: "true"/"false"

0118 |  | Guest extension?

Value: "true"/"false"

0119 |  | Diversion time long

Value range: 0 – 255

0120 |  | Diversion time short

Value range: 0 – 255

0121 |  | DTMF to instrument?

Value: "true"/"false"

0122 |  | Long ring bursts?

Value: "true"/"false"

0123 |  | Repeated call diversion?

Value: "true"/"false"

0124 |  | Call waiting tone for non system instruments?

Value: "true"/"false"

0125 |  | Voice mail extension?

Value: "true"/"false"

0139 |  | Filter coefficient

Value range: 1 – 99

0140 |  | Transmission group
0140
GUI | Value
InitialValue used for all types of ELUs /BTU-A on short trunk lines BTU-D | 0 (default)
BTU-A on medium trunk lines | 1
BTU-A on long trunk lines | 2
2-wire tie lines (BTU-C/ BTU-E) | 3
4-wire tie lines (BTU-E) | 4
Reserved for special market requirements | 5-6
No transmission adaptation | 7

0141 |  | Relative sending level

Value: -12 to 6 , (steps: 0,1 dBr), 3 dBr (default)

0142 |  | Relative receiving level

Value: -12 to 6 , (steps: 0,1 dBr), 3 dBr (default)

0143 |  | Line break time for ELU-A

Value range: 0 – 255, * 50 milliseconds

0144 |  | Hot line delay time

Value range: 0 – 250

0145 |  | Relay control
0145
GUI | Value
No functions(default) | "" empty string
Follows bell | 1
Follows buys state of instrument | 2
Follow message LED | 3

0146 |  | Meter info allowed on display?

Value: "true"/"false"

0147 |  | Type of meter info
0147
GUI | Value
display nothing (function disabled) | 0
display duration of call | 1
display number if metering pulses | 2
display real cost in local currency | 3 (default)

0148 |  | Automatic display of metering info?

Value: "true"/"false"

0149 |  | Number secrecy to public network?

Value: "true"/"false"

0150 |  | Individual charging?

Value: "true"/"false"

0151 |  | Tenant group

Value Range: 0 – 15

0152 |  | Override LCR?

Value: "true"/"false"

0153 |  | Direct carrier access?

Value: "true"/"false"

0154 |  | Limit routing choices LCR

0155 |  | Disable call state message to line?

Value: "true"/"false"

0156 |  | Direct diversion at external calls?

Value: "true"/"false"

0157 |  | Diversion on no reply external calls?

Value: "true"/"false"

0158 |  | Diversion on busy at external calls ?

Value: "true"/"false"

0159 |  | Direct diversion at internal calls?

Value: "true"/"false"

0160 |  | Password check at message retrieving?

Value: "true"/"false"

0161 |  | Music channel in hold state?

Value: "true"/"false"

0162 |  | Terminal type
0162
GUI | Value
(default) | 0
general 3.1kHz audio/ orig.non ISDN | 1
group 3 fax 3.1kHz audio/ orig.non ISDN | 2
modem 3.1kHz audio/ orig.non ISDN | 3
fax 3.1kHz audio/ orig.non ISDN | 3

0163 |  | RTR from extension enabled?

Value: "true"/"false"

0164 |  | DID to extension enabled?

Value: "true"/"false"

0165 |  | Diversion on no reply to slave?

Value: "true"/"false"

0166 |  | Slave always logged on?

Value: "true"/"false"

0167 |  | Ring on master and slave?

Value: "true"/"false"

0168 |  | Use ACD key layout
0168
GUI | Value
Business layout | 0
ACD key layout with clerical key | 1
ACD key layout without clerical key | 2

0169 |  | Directory number subscribed in PSTN?

Value: "true"/"false"

0170 |  | Number/name secrecy to corporate network?

Value: "true"/"false"

0171 |  | Travelling Class Mark

Value Range: 0 – 7

0172 |  | Fixed diversion destination for internal calls, if cordless/IP-Instrument is not available

Value: 4 digits (0-9,*,#); directory number

0173 |  | Fixed diversion destination for external calls, if cordless/IP-Instrument is not available

Value: 4 digits (0-9,*,#); directory number

0174 |  | Alarm group

Value Range: 0 – 7

0175 |  | Use as CTI operator instrument?

Value: "true"/"false"

0176 |  | Call diversion to corporate network allowed?

Value: "true"/"false"

0177 |  | Initiate callback in corporate network?

Value: "true"/"false"

0178 |  | CallList allowed?

Value: "true"/"false"

0179 |  | TCD suffix dialling-day COS

Value Range: 0 – 8

0180 |  | TCD suffix dialling-night COS

Value Range: 0 – 8

0181 |  | Permanent immediate answer allowed?

Value: "true"/"false"

0182 |  | Network intrusion?

Value: "true"/"false"

0183 |  | Directory book allowed

Value: "true"/"false"

0184 |  | Individual external diversion at internal calls

Value: "true"/"false"

0185 |  | Individual external diversion at external calls

Value: "true"/"false"

0186 |  | Handle Cordless Display Texts?

Value: "true"/"false"

0187 |  | Expensive Route Warning Tone

Value: "true"/"false"

0188 |  | Voice transmission quality

Value range: 1 – 4

0189 |  | Conversation recording allowed

Value: "true"/"false"

0190 |  | Switch to non-IP network allowed ?

Value: "true"/"false"

0191 |  | Call cabin extension

Value: "true"/"false"

0192 |  | Multiple Music on hold source number

Value: 0-12

Initial value: 0 (default)

0193 |  | Automatic Redial allowed?

Value: "true"/"false"

0501 |  | Access to common mailbox ?

Value: "<a<XX>>"

Whereas a = "0","1"

XX = 0-15

Example:"0000101011110101"

0502 |  | Notification method

Value range: 0-2

0 | Function disabled
1 | Full notification
2 | Brief notification

0503 |  | Notification number

Value: 24 digits

0504 |  | Notification time

Value: "true"/"false"

0505 |  | Activate notification ?

Value: "true"/"false"

0701 |  | Registration password

Value: 20 characters Default: empty

0702 |  | Client IP address

Value: 0.0.0.0 - 255.255.255.255 Default: 0.0.0.0

4801 |  | Member of loudspeaker paging group 0 ?

Value: "true"/"false"

4802 |  | Member of loudspeaker paging group 1 ?

Value: "true"/"false"

4803 |  | Member of loudspeaker paging group 2 ?

Value: "true"/"false"

4804 |  | Member of loudspeaker paging group 3 ?

Value: "true"/"false"

4805 |  | Member of loudspeaker paging group 4 ?

Value: "true"/"false"

4806 |  | Member of loudspeaker paging group 5 ?

Value: "true"/"false"

4807 |  | Member of loudspeaker paging group 6 ?

Value: "true"/"false"

4808 |  | Member of loudspeaker paging group 7 ?

Value: "true"/"false"

4809 |  | Loudspeaker paging volume

5630 |  | Assign master/slave

Value: 4 digits (0-9,*,#); directory number

5801 |  | Show total survey

Value: "true"/"false"

##### Attribute (DirNum)

Value: 4 digits (0-9,*,#); directory number

#### MO(ISN)

##### Attribute (ISN_<XX>)

Whereas XX = 0 to 81

Value: 0 to 24 digits (0-9,*,#);

0202 |  | Allocate resources for individual short numbers

Value: "true"/"false"

#### MO(PROGKEY)

0201 |  | Allocate resources for programmable keys

Value: "true"/"false"

Note

Use identifier PK_2 instead of PK_02!

##### Attribute (PK_<XX>)

Whereas XX = 0 to 82

Value has following format: "Value(<a>,<b>,<c>,<d>)"

- Command(0301) = a
- Command(0302) = b
- Command(0303) = c
- Command(0304) = d

0301 |  |
0301
GUI | Value
Name Selection (Default) | 10
Suffix Dialing | 11
External Line | 12
Supervision | 13
Intercom | 14
Voice Paging | 15
ACD Group | 16
ACD Supervision | 17
Common Mailbox-supervision | 18
Slave Supervision | 19
R-key | 25
Busy Line 2 / Free 2nd Access | 26
Conference | 27
Immediate Answer | 28
ACD Ready | 29
Account Code | 30
ACD Clerical | 31
ACD Help | 32
Operator – Hold | 33
External Voice Mailbox | 34
Common Hold | 35
Transfer | 36
Save/Redial | 37
Read& | 38
Enter | 39
Number Secrecy | 40
MCID key | 41
Logon/off Slave | 43
ACD Pause | 44
Conv. Recording | 45
Key function

0201 |  | Allocate resources for programmable keys

Value: "true"/"false"

0302 |  | Number/ID

Value: Number,

0 – 2 digits (0 – 7)

0 – 4 digits (0 – 9,*,#)

0303 |  | Ringing alternative

Value Range: 0 – 5

0304 |  | ACD-group priority

Value Range: 0 – 7

### BMS Managed Objects (TrunkMgrMO)

#### TrunkMO(<variable name>)

The variable name can be any identifier beginning with an alphabetical character, followed by any number of (alphabetical or numeric) characters.

1001 |  | Facility COS

Value Range: 0 – 15

1002 |  | Traffic group

Value Range: 0 – 15

1003 |  | TCD-day COS

Value Range: 0 – 8

1004 |  | TCD-night COS

Value Range: 0 – 8

1005 |  | Common abbreviated number COS

Value Range: 0 – 3

1006 |  | Call back allowed?

Value: "true"/"false"

1007 |  | Break-in allowed?

Value: "true"/"false"

1008 |  | Camp-on to answering position?

Value: "true"/"false"

1009 |  | Reroute on answering position barred?

Value: "true"/"false"

1010 |  | Reroute on answering position blocked?

Value: "true"/"false"

1011 |  | Reroute on answering position vacant?

Value: "true"/"false"

1012 |  | Reroute on answering position busy?

Value: "true"/"false"

1013 |  | Dial tone to extension?

Value: "true"/"false"

1014 |  | Result tones to parent exchange?

Value: "true"/"false"

1015 |  | Pre-digits for number analysis

Value: 1-4 digits

1016 |  | Reroute on no answer?

Value: "true"/"false"

1017 |  | Reroute on incomplete number?

    Value: "true"/"false"

1018 |  | Subsystem to PBX?

Value: "true"/"false"

1020 |  | Pick up parked trunk?

Value: "true"/"false"

1022 |  | Voice info to trunk allowed?

Value: "true"/"false"

1023 |  | Trunk line type
1023
GUI | Value
Trunk to a public exchange (PE) | 0
Trunk from a public exchange with direct in-dialing (INDIALING) | 1
Trunk to a private exchange/ tie line (TIE LINE) | 2

1024 |  | Simplified DISA at day?

Value: "true"/"false"

1025 |  | Simplified DISA at night?

Value: "true"/"false"

1028 |  | LCR analysis required?

Value: "true"/"false"

1029 |  | Tenant group

Value range: 0-15

1031 |  | Answer by external line key allowed?

Value: "true"/"false"

1032 |  | Trunk impedance adaption

Value: "true"/"false"

1033 |  | Impedance adaption for transit calls

Value: "true"/"false"

1034 |  | Public dial tone to extension?

Value: "true"/"false"

1036 |  | Type of IBERCOM network connection

1039 |  | Multiple Music on hold source number

Value range: 0-12

1101 |  | Answering position at day

Value: 0-4 digits (0-9,*,#)

1102 |  | Answering position at night

Value: 0-4 digits (0-9,*,#)

1103 |  | Reroute position at day

Value: 0-4 digits (0-9,*,#)

1104 |  | Reroute position at night

Value: 0-4 digits (0-9,*,#)

1109 |  | Common announcement interruptable

Value: "true"/"false"

1201 |  | Line signal scheme
1201
Value | GUI
01 | Standard (simulates analogue telephone)
02 | AGF/AXE with periodic end signal *)
03 | AGF/AXE without periodic end signal *)
04 | A204 with periodic end signal *)
05 | A204 without periodic end signal *)
06 | Australia standard *)
07 | Australia step by step *)
08 | Sweden E&M signaling *)
09 | Continuous E&M signaling A-format *)
10 | Continuous E&M signaling D-format *)
11 | Discontinuous E&M signaling *)
12 | DC-loop signaling *)
13 | Denmark KTAS
14 | Sweden decadic DID (ANSA 134 05) *)
15 | Australia decadic & MFC DID *)
17 | Paging E&M signaling according to ESPA
18 | Holland ALS70 manual lines *)
19 | Holland ALS70 DID *)
20 | Standard with loop break detection
21 | Standard with detection of disconnection tone
22 | Standard with pol. rev. on answer
24 | New Zealand with fast guard facility *)
25 | New Zealand both way with decadic DID *)
26 | Brazil loop DID *)
27 | Spain standard
28 | AXE analogue SS with periodic end signal *)
29 | AXE analogue SS without periodic end signal *)
30 | AXE analogue SS and direct in-dialing (ANSA 134 05) *)
31 | Italy decadic direct in-dialing
34 | Spain with pol. reversal as clearing signal
35 | Austria standard *)
36 | Austria decadic direct in-dialing *)
37 | Austria 12 kHz direct in-dialing with EOS signal *)
38 | Austria 12 kHz direct in-dialing without EOS signal *)
39 | Australia with pol. reversal as clearing signal *)
40 | Belgium analogue DID *)
41 | U.K. ground start *)
42 | U.K. loop start guarded clear *)
43 | U.K. loop start disconnect clear *)
44 | CEPTL 1
45 | CAILHO-discontinuous
46 | SSAC 15 -A
47 | Brazil DID
48 | Egypt DC-loop tie line lass-PSTN
60 | CAS Sweden manual (14101/14301) *)
61 | CAS Sweden DID (ANSA 14401) *)
65 | CAS Italy decadic direct in-dialing *)
66 | CAS Spain MFE direct in-dialing incoming call *)
67 | CAS Spain MFE at outgoing call *)
69 | CAS MFC signaling R2 (CCITT) direct in-dialing or decadic direct in-dialing *)
70 | CAS Belgium
71 | Transmission test
72 | CAS Czech K-sig DID
74 | CAS Italy manual lines *)
75 | CAS Denmark KTAS P1 outgoing DTMF with B-answer *)
76 | CAS Denmark KTAS C1+C2 incoming MFC *)
77 | CAS Denmark KTAS P1+C1+C2 outgoing DTMF incoming MFC with B-answer *)
78 | CAS Denmark KTAS P1 outgoing DTMF without B-answer *)
79 | CASDenmark KTAS P1+C1+C2 outgoing DTMF incoming MFC without B-answer *)
80 | CAS Holland direct in-dialing *)
81 | CAS Holland manually *)
82 | CAS Brazil CCITT R2 MFC/DTMF
83 | CAS Brazil discontinuous E&M
84 | CAS Brazil continuous E&M
85 | CAS Brazil AXE standard
86 | CAS China #1

1301 |  | Incoming digit transmission

1302 |  |
1302
Value | GUI
0 | Decadic impulsing
1 | DTMF
2 | MFC
3 | No sending of digits
4 | MFE1 (2/5)
5 | MFE2 (2/6)

1307 |  | PTS-signal from parent exchange?

Value: "true"/"false"

1308 |  | PTS-signal from parent exchange = dial tone?

Value: "true"/"false"

1309 |  | PTS-signal to parent exchange = dial tone?

Value: "true"/"false"

1312 |  | MFC signal scheme

Value range: 00-15

1312
Value | GUI
0 | Standard R2
1 | Simplified R2
2 | Finnish R2
3 | Norwegian R2
4 | Mexican R2
5 | Australia R2
6 | Belgian simpl.R2
7 | Malaysia R2
8 | Brazil R2
9 | Brazil LME
10 | China R2
11 | Israel R2

1313 |  | DTMF signal scheme

Value: 00-00

1314 |  | Type of dial tone receiver, TRC

Value: 00-00

1315 |  | MFE number plan for CLL

Value: 00-15

1316 |  | Request A-number in MFC?

Value: "true"/"false"

1401 |  | Number of digits with long dial supervision

Value Range: 0 – 9

1402 |  | Time supervision of long register sign. alt. MFC/MFE outgoing

Value: 3-255 seconds

1403 |  | Time supervision of short register sign. alt. MFC/MFE outgoing

Value: 3-255 seconds

1404 |  | Wait time before start to send digits when no PTS

Value: 0-255 seconds

1406 |  | Wait time before ring back/rerouting at not answered calls

Value: 0 – 255

1407 |  | Maximum hold time

Value range: 0 – 255

1408 |  | Minimum speech time for not increasing disturbance counter

Value range: 0 – 255

1409 |  | Time for recall on transfer before answer

Value range: 0 – 255

1410 |  | Time for recall on camp-on

Value range: 0 – 255

1411 |  | Time supervision for first digit at automatic incoming traffic

Value range: 0 – 255

1412 |  | Time supervision between digits at automatic incoming traffic

Value range: 0 – 255

1413 |  | Time supervision of answer at automatic incoming traffic

Value range: 0 – 255

1414 |  | Length detection first PTS

Value range: 01-20

1415 |  | Length detection second PTS

Value range: 01-20

1501 |  | Call meter for trunk?

Value: "true"/"false"

1601 |  | CEPT-DTMF tone receiver level

Value range: -15.0 .. 40.0 dBm0 step 0.5

1602 |  | ETOE-DTMF tone receiver level

Value range: -15.0.. 45.0 dBm0 step 0.5

1603 |  | Dial tone receiver level

Value range: -15.0.. 40.0 dBm0 step 0.5

1604 |  | MFC/MFE tone receiver level

Value range: -15.0.. 45.0 dBm0 step 0.5

1605 |  | MFC/MFE tone sending level

Value range: -3.0.. 20.0 dBm0 step 0.5

1610 |  | Relative sending level

Value range: -12.0.. 6.0 dBm0 step 0.1

1611 |  | Relative receiving level

Value range: -12.0.. 6.0 dBm0 step 0.1

1612 |  | Transmission group
1612
Value | GUI
0 | Initial value, used for all types of ELUs, BTU-A on short trunk lines BTU-D
1 | BTU-A on medium trunk lines
2 | BTU-A on long trunk lines
3 | 2-wire tie lines (BTU-C, BTU-E)
4 | 4-wire tie lines (BTU-E)
5-6 | Reserved for special market requirements
7 | No transmission adaptation

1613 |  | Relative sending level during DTMF

Value range: -12.0.. 6.0 dBm0 step 0.1

1801 |  | Common number at automatic outgoing/incoming traffic

Value: 0 – 4 digits (0 – 9, *, #)

1802 |  | Pre-digits at automatic incoming traffic

Value: 0 – 2 digits (0 – 9, *, #)

1803 |  | Irrelevant digits at automatic incoming traffic

Value Range: 0 – 3

1019 |  | Night-switching group

Value Range: 0 – 8

1030 |  | Public number group

Value Range: 0 – 31

1035 |  | Travelling class mark (TCM)

Value Range: 0 – 7

1105 |  | Common voice announcement at day

Value: empty, 0 - 63

1106 |  | Common voice announcement at night

Value: empty, 0 - 63

1107 |  | Busy voice announcement at day

Value: empty, 0 - 63

1108 |  | Busy voice announcement at night

Value: empty, 0 - 63

1110 |  | 1st, choice CN reroute position

Value: empty, 0 - 3

1111 |  | 2nd, choice CN reroute position

Value: empty, 0 - 3

1112 |  | 3rd, choice CN reroute position

Value: empty, 0 - 3

1303 |  | Impulse type

Value: empty, 0 - 3

1304 |  | Impulse frequency

Value: 0,1

0 = 10 Hz

1 = 16 Hz

1305 |  | Impulse ratio

Value: 0,1

0 = 33/67

1 = 40/60

1306 |  | Inter digit pause
1306
Value | GUI
00 | 300
01 | 350
02 | 400
03 | 450
04 | 500
05 | 550
06 | 600
07 | 650
08 | 700
09 | 750
10 | 800
11 | 850
12 | 900
13 | 950
14 | 1000
15 | 1050

1311 |  | Number of digits before EOS-signal

Value: 1-4 digits, (0 – 9, *, #)

1317 |  | Complete called party number length

Value = 1-32

1405 |  | Wait time before metering is stopped

Value: 000-255 (0-25.5 s)

1416 |  | Blocking time for outgoing call after disconnection

Value = 00-15, (0-15 seconds)

1417 |  | Length of external inquiry signal

Value = 002-255, (20-2550 ms)

1418 |  | Minimum time for detection of call metering pulses

Value = 002-100 (20-1000 ms)

1419 |  | Minimum supervision time between ringsignals

Value = 01-20 (1-20 s)

1420 |  | Number of disconnection tone bursts

Value = 0-10

1421 |  | Pulse time for disconnection tone burst

Value = 0, 100-1000

1422 |  | Pause time for disconnection tone burst

Value = 0, 100-1000

1423 |  | Time supervision of B-answer
1423
Value | GUI
0 | means no supervision.
1-255 | time supervision in number of seconds.

1502 |  | Tariff number

Value = 0-5

1503 |  | Carrier number

Value = 0-7, Default =0

1606 |  | Disconnection tone receiver level

Value = -10.0..40.0

in steps of 0.5 dB

1607 |  | Call meter type

Value: 0,1

0 = 16 kHz

1 = 10 kHz

1608 |  | Call meter receiver level

Value: 0-7, correspondent to following table

CM 12 | CM 12/16
12 kHz | 12 kHz | 16 kHz
(0) | -19.0 dBu | -21.5 dBu | -19.5 dBu
(1) | -20.0 dBu | -25.0 dBu | -23.0 dBu
(2) | -22.0 dBu | -27.0 dBu | -25.0 dBu
(3) | -24.0 dBu | -31.0 dBu | -29.0 dBu
(4) | -26.0 dBu | -33.0 dBu | -30.5 dBu
(5) | -28.0 dBu | -35.0 dBu | -32.5 dBu
(6) | -30.0 dBu | -38.0 dBu | -36.0 dBu
(7) | -33.0 dBu | -43.0 dBu | -40.5 dBu

1609 |  | Filter coefficient

Value: 98..255, according following table:

Value | Input impedance | Balance impedance
98 | Reserved for test. |
99 | Reserved for test. |
100 | Reserved for test. |
Sweden
101 | 0 + 900//30 | 0 + 900//60
Finland short line
102 | 600 | 390 + 620//100
Finland long line
103 | 270 + 910//120 | 270 + 1200//120
Italy
104 | 600 | 400 + 700//200
Spain |  |
105 | 220 + 775//120 | 220 + 820//120
Austria short BTU-A2
106 | 250 + 833//133 | 250 + 833//133
Standard
107 | 600 | 370 + 620//310
Denmark short
108 | 400 + 500//330 | 270 + 390//91
Denmark long
109 | 400 + 500//330 | 300 + 1000//220
Norway
110 | 120 + 820//110 | 120 + 820//110
Netherlands
111 | 600 | 340 + 422//100
Belgium
112 | 150 + 830//72 | 150 + 830//72
Czech. Rep.
113 | 220 + 820//115 | 220 + 820//115
Austria long BTU-A2
114 | 250 + 833//133 | 220 + 1200//150
Australia
115 | 220 + 820//120 | 220+820//120
4-W tie line BTU-E
116 | 600 | –
Australia DDI BTU-C
117 | 370 + 220//310 | 600
England 1 | New Zealand 1
118 | 370 + 620//310 | 370 + 620//310
England 2 | New Zealand 2
119 | 370 + 620//310 | 300 + 1000//220
Brazil
120 | 900 | 800//50
BTU-E 4-wire
121 | 600 | –
Denmark 3 (+ 6 dB)
122 | 400 + 500//330 | 300 + 1000//220
China
123 | 200 + 680//100 | 200 + 680//100
Switzerland 12 kHz Filter
124 | 220 + 820//115 | 220 + 820//115
Extreme long line
125 | 220 + 820//115 | 620 + 1660//275
126-255 | Reserved for future use. |

1614 |  | Call meter (CML) receiver level

Value = -20 .. 45, in steps of 0.5

1706 |  | Seizure acknowledge

Value: "true"/"false"

1707 |  | PTS-signal?

Value: "true"/"false"

1708 |  | EOS-signal?

Value: "true"/"false"

1709 |  | Answer signal?

Value: "true"/"false"

1710 |  | Seizure acknowledge

Value: "true"/"false"

1711 |  | Value(true)

Value: "true"/"false"

1712 |  | EOS-signal?

Value: "true"/"false"

1717 |  | Answer signal?

Value: "true"/"false"

1718 |  | Blocking on separate E2, M2 wires?

Value: "true"/"false"

1804 |  | DDI number translation

Value Range: 0 – 4

1901 |  | CRC-4 alarm conditions

Value: "true"/"false"

1919 |  | Assigned TEI value

Value range: 0-12

1972 |  | Call Forwarding with Partial Rerouting is subscribed

Value: "true"/"false"

1973 |  | ISDN Stimulus services

Value range: 0-12

0 (default) | no services provided |
3 | Call Hold and 3 Party Conference | Italy
4 | Hook Flash | New Zealand

1974 |  | Type of Screening Indicator

Value: 0-3

6301 |  | Log outgoing calls ?

Value: "true"/"false"

##### Attribute (6302_min ) Log duration time

Value: 0-59

##### Attribute (6302_sec) Log duration time

Value: 0-59

6303 |  | Log minimum meter pulses

6304 |  | Bar outgoing calls?

Value: "true"/"false"

6305 |  | Dialed number: suppress

Value = 0-9999 meter pulses

6306 |  | Log dialled numbers beginning with 0

Value: "true"/"false"

6307 |  | Log dialled numbers beginning with 1

Value: "true"/"false"

6308 |  | Log dialled numbers beginning with 2

Value: "true"/"false"

6309 |  | Log dialled numbers beginning with 3

Value: "true"/"false"

6310 |  | Log dialled numbers beginning with 4

Value: "true"/"false"

6311 |  | Log dialled numbers beginning with 5

Value: "true"/"false"

6312 |  | Log dialled numbers beginning with 6

Value: "true"/"false"

6313 |  | Log dialled numbers beginning with 7

Value: "true"/"false"

6314 |  | Log dialled numbers beginning with 8

Value: "true"/"false"

6315 |  | Log dialled numbers beginning with 9

Value: "true"/"false"

6316 |  | Account code required for COS 0

Value: "true"/"false"

6317 |  | Account code required for COS 1

Value: "true"/"false"

6318 |  | Account code required for COS 2

Value: "true"/"false"

6319 |  | Account code required for COS 3

Value: "true"/"false"

6320 |  | Account code required for COS 4

Value: "true"/"false"

6321 |  | Account code required for COS 5

Value: "true"/"false"

6322 |  | Account code required for COS 6

Value: "true"/"false"

6323 |  | Account code required for COS 7

Value: "true"/"false"

6324 |  | Account code required for COS 8

Value: "true"/"false"

6325 |  | Account code required for COS 9

Value: "true"/"false"

6326 |  | Account code required for COS 10

Value: "true"/"false"

6327 |  | Account code required for COS 11

Value: "true"/"false"

6328 |  | Account code required for COS 12

Value: "true"/"false"

6329 |  | Account code required for COS 13

Value: "true"/"false"

6330 |  | Account code required for COS 14

Value: "true"/"false"

6331 |  | Account code required for COS 15

Value: "true"/"false"

6332 |  | Log minimum cost

Value: 0-999999999, default 0

### BMS Managed Objects (FacilityMgrMO)

#### MO(FacilityAccess)

3102 |  | Name for Loudspeaker paging group 0

Value: all printable characters, length:20/ CHECK:ASB_STRING

3103 |  | Name for Loudspeaker paging group 1

Value: all printable characters, length:20/ CHECK:ASB_STRING

3104 |  | Name for Loudspeaker paging group 2

Value: all printable characters, length:20/ CHECK:ASB_STRING

3105 |  | Name for Loudspeaker paging group 3

Value: all printable characters, length:20/ CHECK:ASB_STRING

3106 |  | Name for Loudspeaker paging group 4

Value: all printable characters, length:20/ CHECK:ASB_STRING

3107 |  | Name for Loudspeaker paging group 5

Value: all printable characters, length:20/ CHECK:ASB_STRING

3108 |  | Name for Loudspeaker paging group 6

Value: all printable characters, length:20/ CHECK:ASB_STRING

3109 |  | Name for Loudspeaker paging group 7

Value: all printable characters, length:20/ CHECK:ASB_STRING

2040 |  | Attenuation factor for loudspeaker paging group 0

2041 |  | Attenuation factor for loudspeaker paging group 1

2042 |  | Attenuation factor for loudspeaker paging group 2

2043 |  | Attenuation factor for loudspeaker paging group 3

2044 |  | Attenuation factor for loudspeaker paging group 4

2045 |  | Attenuation factor for loudspeaker paging group 5

2046 |  | Attenuation factor for loudspeaker paging group 6

2047 |  | Attenuation factor for loudspeaker paging group 7

2048 |  | Override individual volume when using loudspeaker paging group 0

Value: "true", "false"

2049 |  | Override individual volume when using loudspeaker paging group 1

Value: "true", "false"

2050 |  | Override individual volume when using loudspeaker paging group 2

Value: "true", "false"

2051 |  | Override individual volume when using loudspeaker paging group 3

Value: "true", "false"

2052 |  | Override individual volume when using loudspeaker paging group 4

Value: "true", "false"

2053 |  | Override individual volume when using loudspeaker paging group 5

Value: "true", "false"

2054 |  | Override individual volume when using loudspeaker paging group 6

Value: "true", "false"

2055 |  | Override individual volume when using loudspeaker paging group 7

Value: "true", "false"

3001 |  | Day/night initiation

Value: "0000000000000000" - "1111111111111111", Length: 16

3002 |  | Transfer before answer

Value: "0000000000000000" - "1111111111111111", Length: 16

3003 |  | System programming

Value: "0000000000000000" - "1111111111111111", Length: 16

3004 |  | Intrusion

Value: "0000000000000000" - "1111111111111111", Length: 16

3005 |  | Conference

Value: "0000000000000000" - "1111111111111111", Length: 16

3006 |  | Loudspeaker paging group 0

Value: "0000000000000000" - "1111111111111111", Length: 16

3007 |  | Loudspeaker paging group 1

Value: "0000000000000000" - "1111111111111111", Length: 16

3008 |  | Loudspeaker paging group 2

Value: "0000000000000000" - "1111111111111111", Length: 16

3009 |  | Loudspeaker paging group 3

Value: "0000000000000000" - "1111111111111111", Length: 16

3010 |  | Loudspeaker paging group 4

Value: "0000000000000000" - "1111111111111111", Length: 16

3011 |  | Loudspeaker paging group 5

Value: "0000000000000000" - "1111111111111111", Length: 16

3012 |  | Loudspeaker paging group 6

Value: "0000000000000000" - "1111111111111111", Length: 16

3013 |  | Loudspeaker paging group 7

Value: "0000000000000000" - "1111111111111111", Length: 16

3014 |  | Send messages for others

Value: "0000000000000000" - "1111111111111111", Length: 16

3015 |  | Send voice messages

Value: "0000000000000000" - "1111111111111111", Length: 16

3016 |  | Send text messsages

Value: "0000000000000000" - "1111111111111111", Length: 16

3017 |  | Send “call me” messages

Value: "0000000000000000" - "1111111111111111", Length: 16

3018 |  | Provide info for others

Value: "0000000000000000" - "1111111111111111", Length: 16

3019 |  | Provide voice info

Value: "0000000000000000" - "1111111111111111", Length: 16

3020 |  | Provide text info

Value: "0000000000000000" - "1111111111111111", Length: 16

3021 |  | Provide predefined info

Value: "0000000000000000" - "1111111111111111", Length: 16

3022 |  | Day/night system

Value: "0000000000000000" - "1111111111111111", Length: 16

3023 |  | Day/night trunk group 1

Value: "0000000000000000" - "1111111111111111", Length: 16

3024 |  | Day/night trunk group 2

Value: "0000000000000000" - "1111111111111111", Length: 16

3025 |  | Day/night trunk group 3

Value: "0000000000000000" - "1111111111111111", Length: 16

3026 |  | Day/night trunk group 4

Value: "0000000000000000" - "1111111111111111", Length: 16

3027 |  | Day/night trunk group 5

Value: "0000000000000000" - "1111111111111111", Length: 16

3028 |  | Day/night trunk group 6

Value: "0000000000000000" - "1111111111111111", Length: 16

3029 |  | Day/night trunk group 7

Value: "0000000000000000" - "1111111111111111", Length: 16

3030 |  | Day/night trunk group 8

Value: "0000000000000000" - "1111111111111111", Length: 16

3031 |  | Program namecall key

Value: "0000000000000000" - "1111111111111111", Length: 16

3032 |  | Program suffix digit key

Value: "0000000000000000" - "1111111111111111", Length: 16

3033 |  | Program external line key

Value: "0000000000000000" - "1111111111111111", Length: 16

3034 |  | Program supervision key

Value: "0000000000000000" - "1111111111111111", Length: 16

3035 |  | Program dedicated line key

Value: "0000000000000000" - "1111111111111111", Length: 16

3036 |  | Program loudspeaker paging key

Value: "0000000000000000" - "1111111111111111", Length: 16

3037 |  | Program ACD-group key

Value: "0000000000000000" - "1111111111111111", Length: 16

3038 |  | Program busy line key

Value: "0000000000000000" - "1111111111111111", Length: 16

3039 |  | Program conference key

Value: "0000000000000000" - "1111111111111111", Length: 16

3040 |  | Program immediate answer key

Value: "0000000000000000" - "1111111111111111", Length: 16

3041 |  | Program ACD ready key

Value: "0000000000000000" - "1111111111111111", Length: 16

3042 |  | Program R-key

Value: "0000000000000000" - "1111111111111111", Length: 16

3043 |  | Program account code key

Value: "0000000000000000" - "1111111111111111", Length: 16

3044 |  | Program ACD supervision key

Value: "0000000000000000" - "1111111111111111", Length: 16

3045 |  | Program ACD clerical key

Value: "0000000000000000" - "1111111111111111", Length: 16

3046 |  | Program ACD help key

Value: "0000000000000000" - "1111111111111111", Length: 16

3047 |  | Program operator hold key

Value: "0000000000000000" - "1111111111111111", Length: 16

3048 |  | Program external voice mail key

Value: "0000000000000000" - "1111111111111111", Length: 16

3049 |  | Program malicious call id key

Value: "0000000000000000" - "1111111111111111", Length: 16

3050 |  | Program number secrecy key

Value: "0000000000000000" - "1111111111111111", Length: 16

3052 |  | Program common message key

Value: "0000000000000000" - "1111111111111111", Length: 16

3053 |  | Program logon / out slave key

Value: "0000000000000000" - "1111111111111111", Length: 16

3054 |  | Program supervise slave key

Value: "0000000000000000" - "1111111111111111", Length: 16

3055 |  | Prog ACD pause key

Value: "0000000000000000" - "1111111111111111", Length: 16

3056 |  | Program recording key

Value: "0000000000000000" - "1111111111111111", Length: 16

3060 |  | Room status view

Value: "0000000000000000" - "1111111111111111", Length: 16

3061 |  | Check in/out

Value: "0000000000000000" - "1111111111111111", Length: 16

3062 |  | Wakeup ordering

Value: "0000000000000000" - "1111111111111111", Length: 16

3063 |  | Wakeup for others

Value: "0000000000000000" - "1111111111111111", Length: 16

3064 |  | Paging

Value: "0000000000000000" - "1111111111111111", Length: 16

3065 |  | Common hold

Value: "0000000000000000" - "1111111111111111", Length: 16

3066 |  | Handle return messages

Value: "0000000000000000" - "1111111111111111", Length: 16

3067 |  | Control messages for others

Value: "0000000000000000" - "1111111111111111", Length: 16

3068 |  | Print ACD statistics

Value: "0000000000000000" - "1111111111111111", Length: 16

3069 |  | Reminder ordering

Value: "0000000000000000" - "1111111111111111", Length: 16

3070 |  | Block room to room / DID traffic

Value: "0000000000000000" - "1111111111111111", Length: 16

3071 |  | External voice mail indication

Value: "0000000000000000" - "1111111111111111", Length: 16

3072 |  | Silent intrusion

Value: "0000000000000000" - "1111111111111111", Length: 16

3073 |  | Alarm extension

Value: "0000000000000000" - "1111111111111111", Length: 16

3074 |  | Read alarm

Value: "0000000000000000" - "1111111111111111", Length: 16

3075 |  | Read own meter

Value: "0000000000000000" - "1111111111111111", Length: 16

3076 |  | Read other’s meter

Value: "0000000000000000" - "1111111111111111", Length: 16

3077 |  | Print other’s meter

Value: "0000000000000000" - "1111111111111111", Length: 16

3078 |  | Reset other’s meter

Value: "0000000000000000" - "1111111111111111", Length: 16

3079 |  | Malicious call id

Value: "0000000000000000" - "1111111111111111", Length: 16

3080 |  | Receive messages

Value: "0000000000000000" - "1111111111111111", Length: 16

3081 |  | Access to DISA

Value: "0000000000000000" - "1111111111111111", Length: 16

3082 |  | Bypass Call diversion

Value: "0000000000000000" - "1111111111111111", Length: 16

3083 |  | Day/night ACD group 0

Value: "0000000000000000" - "1111111111111111", Length: 16

3084 |  | Day/night ACD group 1

Value: "0000000000000000" - "1111111111111111", Length: 16

3085 |  | Day/night ACD group 2

Value: "0000000000000000" - "1111111111111111", Length: 16

3086 |  | Day/night ACD group 3

Value: "0000000000000000" - "1111111111111111", Length: 16

3087 |  | Day/night ACD group 4

Value: "0000000000000000" - "1111111111111111", Length: 16

3088 |  | Day/night ACD group 5

Value: "0000000000000000" - "1111111111111111", Length: 16

3089 |  | Day/night ACD group 6

Value: "0000000000000000" - "1111111111111111", Length: 16

3090 |  | Day/night ACD group 7

Value: "0000000000000000" - "1111111111111111", Length: 16

3091 |  | Day/night all ACD groups

Value: "0000000000000000" - "1111111111111111", Length: 16

3092 |  | Individual programming

Value: "0000000000000000" - "1111111111111111", Length: 16

3093 |  | Individual external diversion

Value: "0000000000000000" - "1111111111111111", Length: 16

3094 |  | Conversation recording

Value: "0000000000000000" - "1111111111111111", Length: 16

#### MO(MessageWelcome)

8501 |  | Individual message welcome 1

##### Attribute (8501_0)

Value range: "0" - "31"

to

##### Attribute (8501_15)

Value range: "0" - "31"

8502 |  | Announce directory number?

##### Attribute (8502_0)

Value: "true", "false"

to

##### Attribute (8502_15)

Value: "true", "false"

8503 |  | Individual message welcome 2

##### Attribute (8503_0)

Value range: "0" - "31"

to

##### Attribute (8503_15)

Value range: "0" - "31"

8510 |  | Individual message when retrieving

##### Attribute (8510_0)

Value range: "0" - "15"

to

##### Attribute (8510_15)

Value range: "0" - "15"

8512 |  | Exit position

##### Attribute (8512_0)

Value: max. 4 digits (0-9,*,#)

to

##### Attribute (8512_15)

Value: max. 4 digits (0-9,*,#)

#### ACD System

2057 |  | Follow me/Diversion to ACD

Value: "true", "false"

2081 |  | Modified business key layout

Value: "true", "false"

2083 |  | Terminate ACD calls with group key

Value: "true", "false"

2086 |  | Non blocked ACD

Value: "true", "false"

3704 |  | Queue tone?

Value: "true", "false"

3705 |  | ACD-I/O monitor frequence

Value range: "0" - "9"

3706 |  | ACD-I/O port for PC-graph

,"",CHECK:NOCHECK/ TYPE:CARD_INDEX

3708 |  | ACD-I/O port for MS

,"",CHECK:NOCHECK/ TYPE:CARD_INDEX

3709 |  | New agent = last?

Value: "true", "false"

3710 |  | Pause time

Value range: "1" - "30"

3711 |  | Non ACD callcode request?

Value: "true", "false"

3712 |  | Display clerical time?

Value: "true", "false"

#### MO(MessageSystem)

4301 |  | Max time for speech message

Value range: "0" - "255"

4302 |  | Max time for speech info

Value range: "0" - "255"

4303 |  | Max time for speech anno

Value range: "0" - "255"

4304 |  | Time to keep message

Value range: "1" - "99"

4304 |  | Time to keep message

Value range: "0" - "99"

4305 |  | Voice message quality
4305
Value | GUI
"0" | normal
"1" | high

4306 |  | Voice information quality
4306
Value | GUI
"0" | normal
"1" | high

4307 |  | Voice answer quality
4307
Value | GUI
"0" | normal
"1" | high

4308 |  | No answer to sender (days)

Value range: "0" - "99"

4308 |  | No answer to sender (days)

Value range: "0" - "99"

4309 |  | Keep answered call me

Value range: "0" - "99"

4310 |  | Keep answered voice

Value range: "0" - "99"

4311 |  | Keep answered text

Value range: "0" - "99"

4312 |  | Short message store

Value: "true", "false"

4314 |  | Simult retrievings

Value range: "1" - "16"

4315 |  | Silent detect level VMU-HD

Value range: "-70" - "-20"

4316 |  | Silent detect time VMU-HD

1. Value range: "", "5" - "30"

4317 |  | Play date/time info prior to message

Value: "true", "false"

4318 |  | Number of days to keep archived messages

Value range: "0" - "99"

4319 |  | Number of days to keep heard messages

Value range: "0" - "10"

4320 |  | Notification scheduling profile

Value range: 2-6

Table shows the 6 notification scheduling profile:

SelectionValue | Scheduling profile
"2" | 10 min nonlinear
"3" | 20 min nonlinear
"4" | 30 min linear
"5" | 60 min linear
"6" | 90 min linear

4321 |  | Maximum number of active OCN users

Value: {5,10,20,30,40,50} decimal

4322 |  | Maximum number of OCN trunks

Value range: 1-8 (decimal)

4323 |  | Number of OCN repetitions

Value range: 0-10 (decimal)

4324 |  | OCN user acknowledgement time

Value range: 1-255 (decimal)

Default value: 60

4501 |  | Predefined info - Text

##### Attribute (4501_1)

Value: all printable characters, Length: 35

to

##### Attribute (4501_7)

Value: all printable characters, Length: 35

4502 |  | Predefined info - Meaning of digits 1-4

##### Attribute (4502_1)

Value range: "1" - "3"

to

##### Attribute (4502_7)

Value range: "1" - "3"

4503 |  | Predefined info - Text for cordless

##### Attribute (4503_1)

Value: all printable characters, Length: 35

to

##### Attribute (4503_7)

Value: all printable characters, Length: 35

8301 |  | Reminder ringing time

Value range: "1" - "59"

8302 |  | Reminder pause time

Value range: "1" - "5"

8303 |  | Reminder attempts

Value range: "1" - "5"

8304 |  | Reminder answer anno

Value: max. 4 digits (0-9,*,#)

##### Attribute (8601_1 ) null

Value range: "", "0" - "31"

##### Attribute (8601_2 ) null

Value range: "", "0" - "31"

##### Attribute (8601_3 ) null

Value range: "", "0" - "31"

##### Attribute (8602_1 ) null

Value: "true", "false"

##### Attribute (8602_2 ) null

Value: "true", "false"

##### Attribute (8602_3) null

Value: "true", "false"

##### Attribute (8603_1) null

Value range: "", "0" - "31"

##### Attribute (8603_2) null

Value range: "", "0" - "31"

##### Attribute (8603_3) null

Value range: "", "0" - "31"

##### Attribute (8604_1 ) null

Value range: "", "0" - "15"

##### Attribute (8604_2) null

Value range: "", "0" - "15"

##### Attribute (8604_3 ) null

Value range: "", "0" - "15"

#### MO(ConferenceSystem)

4901 |  | Number of participants

Value range: "3" - "6"

4902 |  | Number of external lines

Value range: "1" - "5"

4903 |  | Number of PE-lines

Value range: "1" - "5"

#### MO(PagingSystem)

8101 |  | Number of paging digits

Value range: "1" - "4"

8102 |  | Number of display digits

Value range: "0" - "10"

8103 |  | Mode digit

Value range: "0" - "2"

8104 |  | Paging absence?

Value: "true", "false"

8105 |  | Paging channel

Value: trunk or route directory number

8106 |  | Display string

Value: max. 4 digits (0-9,*,#)

8107 |  | End of paging number

Value: "true", "false"

8108 |  | Max paging speech time

Value range: "10" - "255"

8109 |  | Paging meet-me time

Value range: "10" - "255"

8110 |  | Paging progress time

Value range: "1" - "60"

8112 |  | Mode digit meet-me

Value range: "", "0" - "9"

8113 |  | Mode digit external

Value range: "", "0" - "9"

8114 |  | Mode digit call-me

Value range: "", "0" - "9"

8115 |  | Mode digit group

Value range: "", "0" - "9"

8116 |  | Mode digit display

Value range: "", "0" - "9"

8117 |  | Mode digit speech

Value range: "", "0" - "9"

8118 |  | Mode digit external call

Value range: "", "0" - "9"

8201 |  | Receiver dirno

##### Attribute (8201_1)

Value: max. 4 digits (0-9,*,#)

to

##### Attribute (8201_250)

Value: max. 4 digits (0-9,*,#)

8202 |  | Search code

##### Attribute (8202_1)

Value: max. 4 digits (0-9,*,#)

to

##### Attribute (8202_250)

Value: max. 4 digits (0-9,*,#)

8203 |  | Receiver type

##### Attribute (8203_1)

to

##### Attribute (8203_250

8203
Value | GUI
"0" | ‘Bleeper’ type rec., no display
"1" | Display rec. for call-me paging
"2" | Rec. with speech poss., no display
"3" | Rec. with speech poss., display
"4" | Group call, no display
"5" | Group call, display
"6" | Display rec. for meet-me paging

)

#### MO(NetworkSystem)

9001 |  | Call setup version at network CBack

9002 |  | Active time for ’CBack on busy’ initPBX

Value range: "0005" - "0855"

in steps of 5 must be smaller than (9004)

9003 |  | Active time for ’CBack on free’ initPBX

Value range: "0005" - "0855"

in steps of 5 must be smaller than (9005)

9004 |  | Active time for ’CBack on busy’ superPBX

Value range: "0010" - "0900" in steps of 5

Must be larger than (9002)

9005 |  | Active time for ’CBack on free’ superPBX

Value range: "0010" - "0900" in steps of 5

Must be larger than (9003)

9006 |  | Maxringtime at the init extension for CBack calls

Value range: "1" - "255"

2071 |  | ISID of external voice mailbox

Value range: "", "0" - "99"

2072 |  | MD110 release version of CN

2073 |  | Removed digits for composing A or B number

Value range: "0" - "3"

2074 |  | Local private code for composing A or B number

Value: max. 4 digits (0-9,*,#

2077 |  | First central answering position

Value: max. 8 digits (0-9,*,#)

2078 |  | Second central answering position

Value: max. 8 digits (0-9)

2079 |  | Third central answering position

Value: max. 8 digits (0-9)

2084 |  | Type of network call handling

2085 |  | PBX protocol identifier

Value range: "0" - "0xFF"

2087 |  | Transit counter

Value range: "1" - "31"

#### MO(CTISystem)

8901 |  | CTI port

Value: "SSIII" SS = Slot, III = Individual

8902 |  | CTI route timeout

Value range: "1" - "30"

#### MO(Hotel)

8001 |  | Room status change

Value Range: 00 ..23

8002 |  | Room to room bar

Value Range: 00 ..23

8003 |  | Room to room open

Value Range: 00 ..23

8004 |  | Hotel answering position

Value: 4 digits (0-9,*,#); directory number

8006 |  | Wake-up ring time

Value range:0..59

Initial value = 30

8007 |  | Wake-up ring pause

Value range:1..5

Initial value = 3

8008 |  | Wake-up ring attempts

Value range: A..Z

Initial value = " "

8009 |  | Wake-up language 1

Value range: A..Z

Initial value =" "

8010 |  | Wake-up language 2

Value range: A..Z

Initial value = " "

8011 |  | Wake-up language 3

Value range: A..Z

Initial value = " "

8012 |  | Wake-up answer anno 1

Value: 4 digits (0-9,*,#); directory number

8013 |  | Wake-up answer anno 2

Value: 4 digits (0-9,*,#); directory number

8014 |  | Wake-up answer anno 3

Value: 4 digits (0-9,*,#); directory number

8015 |  | Wake-up order ref 1

Value: 4 digits, Format iijj,ii= { 00,01} jj={01-32}

8016 |  | Wake-up order ref 2

Value: 4 digits, Format iijj,ii= { 00,01} jj={01-32}

8017 |  | Wake-up order ref 3

Value: 4 digits, Format iijj,ii= { 00,01} jj={01-32}

8018 |  | Wake-up order time 1

Value: "true"/"false"

8019 |  | Wake-up order time 2

Value: "true"/"false"

8020 |  | Wake-up order time 3

Value: "true"/"false"

8021 |  | RTR/DID time status

Value range: 1 .. 3

Initial value: 2

8021
GUI | Value
RTR+DID | 1
RTR | 2
DID | 3

8030 |  | Guest instrument key A

Values range: A-E

8031 |  | Guest instrument key B

Values range: A-E

8032 |  | Guest instrument key C

Values range: A-E

8033 |  | Guest instrument key D

Values range: A-E

8034 |  | Guest instrument key E

Values range: A-E

8035 |  | Guest instrument key F

Values range: A-E

8036 |  | Guest instrument key G

Values range: A-E

MO(CarMan)

##### Attribute (CarrierExists_0) Create/Delete Carrier

Value: "true"/"false"

##### Attribute (CarrierExists_1) Create/Delete Carrier

Value: "true"/"false"

##### Attribute (CarrierExists_2) Create/Delete Carrier

Value: "true"/"false"

##### Attribute (CarrierExists_3) Create/Delete Carrier

Value: "true"/"false"

##### Attribute (CarrierExists_4) Create/Delete Carrier

Value: "true"/"false"

##### Attribute (CarrierExists_5) Create/Delete Carrier

Value: "true"/"false"

##### Attribute (CarrierExists_6) Create/Delete Carrier

Value: "true"/"false"

##### Attribute (CarrierExists_7) Create/Delete Carrier

Value: "true"/"false"

5623 |  | LCR directory number

Value: 4 digits (0-9,*,#); directory number

2024 |  | Initiate public Dialtone at LCR

Value: "true"/"false"

2034 |  | Initiate dial tone at LCR

Value: "true"/"false"

2035 |  | Predicted call duration

Value:10 digits incl. Decimal point

#### MO(AuthorityCode)

2019 |  | ACOS at authority code

Value range: "0" - "15"

2020 |  | TCD-day at authority code

Value range: "0" - "8"

2021 |  | TCD-night at authority code

Value range: "0" - "8"

2022 |  | Abbreviated number COS at authority code

Value range: "0" - "3"

#### MO(ApplicationIO)

##### Attribute (6401_0) Initiate I/O ports

Address of the I/O port

Value: "SSIII" SS = Slot

III = Individual

##### Attribute (6401_1) Initiate I/O ports

Address of the I/O port

Value: "SSIII" SS = Slot

III = Individual Attribute/

##### Attribute (6402_0) Activate I/O ports?

Value: "true", "false"

##### Attribute (6402_1) Activate I/O ports?

Value: "true", "false"

##### Attribute (6403_0) Format table

##### Attribute (6403_1) Format table

6403
Value | GUI
"0" | No formatting
"1" | Call MD110/standard
"2" | Call (printer)
"3" | Call/hotel (printer)
"4" | Call/hotel ASB150/ht
"5" | Call/hotel MD110/ht
"6" | Call/hotel HIS
"7" | Call/hotel CILHOTEL
"8" | Call/hotel CIL2HOTEL
"9" | Call/hotel CIL3HOTEL
"10" | Call/hotel CIL4HOTEL (R12 only)
"34" | Hotel ASB150/ht (in)
"35" | Hotel MD110/ht (in)
"36" | Hotel HIS (in)
"37" | Hotel CILHOTEL (in)
"64" | Hotel ASB150/ht (bi)
"65" | Hotel MD110/ht (bi)
"66" | Hotel HIS (bi)
"67" | Hotel CILHOTEL (bi)
"68" | Hotel CIL2HOTEL (bi)
"69" | Hotel CIL3HOTEL (bi)
"71" | Hotel CIL4HOTEL (bi) (R12 only)
"70" | Call CTI (out)

##### Attribute (6404_0) Lines per page

Value range: "0" - "99"

##### Attribute (6404_1) Lines per page

Value range: "0" - "99"

##### Attribute (6405_0) I/O time supervision

Value range: "70" - "255"

##### Attribute (6405_1) I/O time supervision

Value range: "70" - "255"

##### Attribute (6406_0) Automatic I/O activation

Value range: "0" - "11"

##### Attribute (6406_1) Automatic I/O activation

Value range: "0" - "11"

##### Attribute (6420_X) Flexible CIL- format

Whereas X = 1 to 30

Application IO
No. | CIL-Data Information | Character
1 | Message code | (2)
2 | Sequence number CIL4 | (3)
3 | Call date CIL4 | (6)
4 | End time CIL4 | (4)
5 | Caller´s number CIL4 | (4)
6 | Call duration CIL4 | (5)
7 | Meter pulses CIL4 | (4)
8 | Dialed access code CIL4 | (4)
9 | Dialed number CIL4 | (24)
10 | Information status 2 CIL4 | (1)
11 | Account code CIL4 | (15)
12 | Authorisation code CIL4 | (4)
13 | Queue time, answer CIL4 | (4)
14 | Information status 1 CIL4 | (1)
15 | Cost CIL4 | (11)
16 | Cost state CIL4 | (1)
17 | Trunk number CIL4 | (4)
18 | Sent access code CIL4 | (4)
19 | Sent number CIL4 | (24)
20 | A-number CIL4 | (20)
21 | Call via facility CIL4 | (1)
22 | Transfer condition CIL4 | (2)
23 | Carriage return/LF | (2)
24 | Sequence number + A HIS | (4)
25 | Hotel ALPHA HIS | (3)
26 | Call date (mmdd) HIS | (4)
27 | Caller´s number HIS | (5)
28 | End time (hhmm) HIS | (4)
29 | Call duration (minutes) HIS | (4)
30 | Called number HIS | (14)
31 | Hotel ALPHA EBC | (3)
32 | Call duration (hhmm/10) ASB | (4)
33 | Information status ASB | (1)
34 | Called number ASB | (20)
35 | Caller´s number DDI | (8)
36 | Space 1....(place reservation) | (1)
37 | Space 5....(place reservation) | (5)
38 | Space 10...(place reservation) | (10)
39 | End time hh:mm:ss | (8)
40 | TAG identifier | (5)

6431 |  | Test protocol port address

Address of the I/O port

Value: "SSIII" SS = Slot, III = Individual

6432 |  | Enable test protocol

Value: "true", "false"

#### MO(AlarmHeartbeat)

7420 |  | Service area id

Value: all printable characters, length:5

7421 |  | Identity of exchange

Value: all printable characters, length:5

7430 |  | Active alarm on?

Value: "true", "false"

7431 |  | Active alarm I/O port

Value: "SSIII" SS = Slot, III = Individual

7432 |  | Active alarm receiver

Value range: "0" - "11"

7433 |  | Active alarm via internal modem?

Value: "true", "false"

7434 |  | Active alarm number

Value: max. 18 digits (0-9,*,#)

7435 |  | Active alarm pause

Value range: "0" - "120"

7436 |  | Active alarm attempts

Value range: "0" - "5"

7437 |  | Max active alarms per day

Value range: "0" - "255"

7440 |  | Heartbeat on?

Value: "true", "false"

7441 |  | Heartbeat I/O port

Value: "SSIII" SS = Slot, III = Individual

7442 |  | Heartbeat receiver

Value range: "0" - "11"

7443 |  | Heartbeat via internal modem?

Value: "true", "false"

7444 |  | Heartbeat number

Value: max. 18 digits (0-9,*,#)

7445 |  | Heartbeat pause

Value range: "0" - "120"

7446 |  | Heartbeat attempts

Value range: "0" - "5"

7447 |  | Heartbeat pace

Value range: "0" - "255"

#### MO(CIL)

6201 |  | Log internal calls?

Value: "true", "false"

6202 |  | Log incoming calls?

Value: "true", "false"

6203 |  | Block log output?

Value: "true", "false"

6204 |  | Digits to log
6204
Value | GUI
"0" | dialed
"1" | sent

6205 |  | Bar outgoing calls for guest

Value: "true", "false"

#### MO(CallMetering)

6701 |  | I/O Port

Value: "SSIII" SS=Slot, III=Individual

6702 |  | Lines/page

Value range: "0" - "255"

6703 |  | Printout header 1

Value: all printable characters, length:50

6704 |  | Printout header 2

Value: all printable characters, length:50

6705 |  | Printout header 3

Value: all printable characters, length:50

6706 |  | Printout header 4

Value: all printable characters, length:50

6710 |  | Currency identifier

Value: all printable characters, length:3

6711 |  | Decimals in cost

Value range: "0" - "4"

6712 |  | Currency id last?

Value: "true", "false"

6713 |  | Cost limit

Value: max. 9 digits including decimals

6720 |  | Operator password

Value: max. 10 digits (0-9,*,#)

#### MO(CarMan)

##### Attribute (CarrierExists_0) Create/Delete Carrier

Value: "true"/"false"

##### Attribute (CarrierExists_1) Create/Delete Carrier

Value: "true"/"false"

##### Attribute (CarrierExists_2) Create/Delete Carrier

Value: "true"/"false"

##### Attribute (CarrierExists_3) Create/Delete Carrier

Value: "true"/"false"

##### Attribute (CarrierExists_4) Create/Delete Carrier

Value: "true"/"false"

##### Attribute (CarrierExists_5) Create/Delete Carrier

Value: "true"/"false"

##### Attribute (CarrierExists_6) Create/Delete Carrier

Value: "true"/"false"

##### Attribute (CarrierExists_7) Create/Delete Carrier

Value: "true"/"false"

5623 |  | LCR directory number

Value: 4 digits (0-9,*,#); directory number

2024 |  | Initiate public Dialtone at LCR

Value: "true"/"false"

2034 |  | Initiate dial tone at LCR

Value: "true"/"false"

2035 |  | Predicted call duration

Value:10 digits incl. Decimal point

#### MO (Carrier_<XX>)

Whereas XX = 0 to 7

8401 |  | Internal access code

Value: 0-4 digits

8402 |  | Predigit for carrier access

Value: 0-4 digits

8403 |  | Billing principle

Value: 0,1 (0=Pulse, 1=Duration)

8430 |  | Customer tariff (cost per pulse) 0

Value: Decimal Number

8431 |  | Customer tariff (cost per pulse) 1

Value: Decimal Number

8432 |  | Customer tariff (cost per pulse) 2

Value: Decimal Number

8433 |  | Customer tariff (cost per pulse) 3

Value: Decimal Number

8434 |  | Customer tariff (cost per pulse) 4

Value: Decimal Number

8435 |  | Customer tariff (cost per pulse) 5

Value: Decimal Number

8405 |  | Detecting carrier access codes

##### Attribute (8405AC_<XX>) Access code

Whereas XX = 0 to 15

Value: 0 to 10 digits

##### Attribute (8405PN_<XX>) Public numbers

Whereas XX = 0 to 15

Value:

8410 |  | Destination number modification

##### Attribute (8410DN_<XX>) Destination number

Whereas XX = 0 to 15

Value:0 to 10 digits

##### Attribute (8410AC_<XX>) Carrier access

Whereas XX = 0 to 15

Value: 0 to 10 digits

##### Attribute (8410DE_<XX>) Delete

Whereas XX = 0 to 15

Value: 0 to 10 digits

8415 |  | Arranging number to send

##### Attribute (8415COMPID_<XX>)

Whereas XX = 0 to 7

Value:0-7, default: empty

8415 number component
Value | GUI
" |
’0’ | B-number
’1’ | External access code
’2’ | Authority code
’3’ | Account code
’4’ | Own extension number
’5’ | Change to DTMF
’6’ | Wait for Proceed To Send tone
’7’ | Delay time

##### Attribute (8415LENGTH_<XX>)

Whereas XX = 0 to 7

##### Attribute (8415DATA_<XX>)

Only for Delay time (8415COMPIDValue=7)

Whereas XX = 0 to 7

Value: 0-30 seconds

8440 |  | Call cost profile

##### Attribute (8440CTS_<XX>)

Whereas XX = 0 to 248

##### Attribute (8440CLT_<XX> )

Whereas XX = 0 to 248

##### Attribute (CTS_Exists_<XX>)

Whereas XX = 0 to 35

Value: "true"/"false"

##### Attribute (PCL_Exists_<XX>)

Whereas XX = 0 to 59

Value: "true"/"false"

Attribute (TCL_Exists_<XX>)

Whereas XX = 0 to 59

Value: "true"/"false"

8420 |  | Open

##### Attribute (8420_<XX>)

Whereas XX = 0 to 15

Value: 1 – open; 2 – closed

8421 |  | Account code

##### Attribute (8421_<XX>)

Whereas XX = 0 to 15

Value: 0-5 digits

8422 |  | Authority code

##### Attribute (8422_<XX>)

Whereas XX = 0 to 15

Value: 0-16 digits

8423 |  | Pulse cost LCR

##### Attribute (8423_<XX>)

Whereas XX = 0 to 15

Value: 10 digits incl. decimal point

8424 |  | Multiplication factors

##### Attribute (8424_<XX>)

Whereas XX = 0 to 15

Value range: 0,0001-999

8425 |  | Discount factor LCR %

##### Attribute (8425_<XX>)

Whereas XX = 0 to 15

Value: 10 digits incl. decimal point

8427 |  | Call cost profile

##### Attribute (8427_CTS_<XX>_<YY>) Cost time scheme index

Whereas XX = 0 to 15

Whereas YY = 0 to 249

Value: index defined in 8440

##### Attribute (8427_CLT_<XX>_<YY>) Cost level table index

Whereas XX = 0 to 15

Whereas YY = 0 to 249

Value: index defined in Cost Level Table (8455/8465)

#### MO (CostTimeScheme_<YY>)

Whereas YY =

8445 |  | Cost time scheme general

##### Attribute (8445DT1_<XX>)

Whereas XX = 0 to 23

Value:

##### Attribute (8445DT2_<XX>)

Whereas XX = 0 to 23

Value:

##### Attribute (8445DT3_<XX>)

Whereas XX = 0 to 23

Value:

#### MO (PulseCostLevel_<YY>)

Whereas YY = 0 to 59

8455 |  | Pulse rate table general (list price)

##### Attribute (8455IP_<XX>)

Whereas XX = 0 to 15

Value: 0 to 10 digits

##### Attribute (8455FQ_<XX>)

Whereas XX = 0 to 15

Value: 0 to 10 digits

#### MO (TimeCostLevel_<YY>)

Whereas YY = 0 to 59

8465 |  | Cost level table general (list price)

cost/s: up to 10 digits

##### Attribute (8465IC_<XX>)

Whereas XX = 0 to 15

Value: 0 to 10 digits

##### Attribute (8465PS_<XX>)

Whereas XX = 0 to 15

Value:0 to 10digits

#### MO(MailboxMan)

5427 |  | Create common mailbox

##### Attribute (Mailbox_0)

to

##### Attribute (Mailbox_15)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted.
If this value is set to a free directory number, the facility is created or altered.

5527 |  | Delete common mailbox number

##### Attribute (Mailbox_0)

to

##### Attribute (Mailbox_15)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted.
If this value is set to a free directory number, the facility is created or altered.

5627 |  | Alter common mailbox directory number

##### Attribute (Mailbox_0)

to

##### Attribute (Mailbox_15)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted.
If this value is set to a free directory number, the facility is created or altered.

#### MO(Mailbox_0)

5627 |  | Alter common mailbox directory number

Value: max. 4 digits (0-9,*,#)

Changes the directory number of this facility.

6501 |  | Directory name

Value: Printable character, length: 35

Changes the directory name of this facility.

5701 |  | BlockedFlag

Value: "true", "false"

8507 |  | Common mailbox welcome 1

Value range: "0" - "15"

8508 |  | Common mailbox welcome 2

Value range: "0" - "15"

8509 |  | Common mailbox welcome 3

Value range: "0" - "15"

8511 |  | Welcome announcement when retrieving from common mailbox

Value range: "0" - "15"

#### MO(IndividualMailboxMan)

5426 |  | Create individual mailbox

##### Attribute (IndividualMailbox_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5526 |  | Delete individual mailbox number

##### Attribute (IndividualMailbox_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5626 |  | Alter individual mailbox directory number

##### Attribute (IndividualMailbox_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

#### MO(IndividualMailbox_0)

5626 |  | Alter individual mailbox directory number

Value: max. 4 digits (0-9,*,#)

Changes the directory number of this facility.

6501 |  | Directory name

Value: Printable character, length: 35

Changes the directory name of this facility.

5701 |  | BlockedFlag

Value: "true", "false"

#### MO(RouteMan)

5401 |  | Create a route

##### Attribute (Route_0)

to

##### Attribute (Route_249)

Value: max. 4 digits (0-9,*,#)

If this value is set to " " the facility is deleted.

5501 |  | Delete a route

##### Attribute (Route_0)

to

##### Attribute (Route_249)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted.

5608 |  | Alter route number

##### Attribute (Route_0)

to

##### Attribute (Route_249)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted.

##### Route_0 can not be deleted

If this value is set to a free directory number, the facility is created or altered.

#### MO(Route_0)

5608 |  | Alter route number

Value: max. 4 digits (0-9,*,#)

Changes the directory number of this facility.

6501 |  | Directory name

Value: Printable character, length: 35

Changes the directory name of this facility.

5701 |  | BlockedFlag

Value: "true", "false"

3201 |  | Route members

##### Attribute (3201_0)

to

##### Attribute (3201_45)

Max. 4 digits

Only trunk directory numbers are allowed

3301 |  | Random Selection

Value: "true", "false"

3302 |  | Callback allowed?

Value: "true", "false"

3303 |  | Predigits

Value: max. 10 digits (0-9,*,#)

3304 |  | First alternative route

Max. 4 digits

Only route directory numbers are allowed

3305 |  | Predigits for first alternative route

Value: max. 10 digits (0-9,*,#)

3306 |  | Second alternative route

Max. 4 digits

Only route directory numbers are allowed

3307 |  | Predigits for second alternative route

Value: max. 10 digits (0-9,*,#)

#### MO(OperatorMan)

5613 |  | Alter operator directory number

##### Attribute (Operator_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. This is not possible for the operator facility.

If this value is set to a free directory number, the facility is created or altered. The operator facility always exists.

#### MO(Operator_0)

5613 |  | Alter operator directory number

Value: max. 4 digits (0-9,*,#)

Changes the directory number of this facility.

6501 |  | Directory name

Value: Printable character, length: 35

Changes the directory name of this facility.

5701 |  | BlockedFlag

Value: "true", "false"

4001 |  | Alternative answer position

Value: max. 8 digits (0-9,*,#)

4003 |  | Answering time

Value range: "15" - "255"

4004 |  | Cyclical selection

Value: "true", "false"

4005 |  | Auto. answer superv. time

Value range: "0" - "11"

4006 |  | Queue announcement time

    Value range: "0" - "255"

4007 |  | Queue announcement reference

Value: "UUVV" UU=1,VV=1-32, 0000 = no reference

4008 |  | Calling of extension at incoming call

Value range: "0" - "1"

4009 |  | Two external lines at operator 3-party

Value: "true", "false"

4010 |  | Two PE-lines at operat. 3-party

Value: "true", "false"

4011 |  | Listening during the announcement

Value: "true", "false"

4012 |  | Sending a ready tone after announcement

Value: "true", "false"

4101 |  | Operator line position

##### Attribute (4101_1)

##### Attribute (4101_2)

##### Attribute (4101_3)

Value: "SSIII" SS = Slot

III = Individual

4102 |  | Operator answer reference

##### Attribute (4102_1)

##### Attribute (4102_2)

##### Attribute (4102_3)

Value: "UUVV" UU=1,VV=1-32

0000 = no reference

4103 |  | Ringburst at queue

##### Attribute (4103_1)

##### Attribute (4103_2)

##### Attribute (4103_3)

Value: "true", "false"

4104 |  | Receiving of tone signals

##### Attribute (4104_1)

##### Attribute (4104_2)

##### Attribute (4104_3)

- Value: "true", "false"

#### MO(CommonBellMan)

5629 |  | Pickup code for common bell

##### Attribute (CommonBell_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. This is not possible for the common bell facility.

If this value is set to a free directory number, the facility is created or altered. The common bell facility always exists.

#### MO(CommonBell_0)

5629 |  | Pickup code for common bell

Value: max. 4 digits (0-9,*,#)

Changes the directory number of this facility.

6501 |  | Directory name

Value: Printable character, length: 35

Changes the directory name of this facility.

5701 |  | BlockedFlag

Value: "true", "false"

6901 |  | Common bell extension

Value: max. 4 digits (0-9,*,#)

#### MO(OwnLocationCodeMan)

5431 |  | Create Own Location Code

##### Attribute (OwnLocationCode_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5531 |  | Delete Own Location Code

##### Attribute (OwnLocationCode_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5631 |  | Alter own location code

##### Attribute (OwnLocationCode_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

#### MO(OwnLocationCode_0)

5627 |  | Alter common mailbox directory number

Value: max. 4 digits (0-9,*,#)

Changes the directory number of this facility.

6501 |  | Directory name

Value: Printable character, length: 35

Changes the directory name of this facility.

5701 |  | BlockedFlag

Value: "true", "false"

#### MO(CallNumStandardMan)

5410 |  | Create call number for standard paging

##### Attribute (CallNumStandard_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted.

If this value is set to a free directory number, the facility is created or altered.

5510 |  | Delete call number for standard paging

##### Attribute (CallNumStandard_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted.

If this value is set to a free directory number, the facility is created or altered.

5617 |  | Alter call number for standard paging

##### Attribute (CallNumStandard_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted.

If this value is set to a free directory number, the facility is created or altered.

#### MO(CallNumStandard_0)

5617 |  | Alter call number for standard paging

Value: max. 4 digits (0-9,*,#)

Changes the directory number of this facility.

6501 |  | Directory name

Value: Printable character, length: 35

Changes the directory name of this facility.

5701 |  | BlockedFlag

Value: "true", "false"

#### MO(CallNumAlternativeMan)

5411 |  | Create call number for alternative paging

##### Attribute (CallNumAlternative_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5511 |  | Delete call number for alternative paging

##### Attribute (CallNumAlternative_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5618 |  | Alter call number for alternative paging

##### Attribute (CallNumAlternative_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

#### MO(CallNumAlternative_0)

5618 |  | Alter call number for alternative paging

Value: max. 4 digits (0-9,*,#)

Changes the directory number of this facility.

6501 |  | Directory name

Value: Printable character, length: 35

Changes the directory name of this facility.

5701 |  | BlockedFlag

Value: "true", "false"

#### MO(CallNumMeetMeMan)

5412 |  | Create answer number for meet-me

##### Attribute (CallNumMeetMeCode_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5512 |  | Delete answer number for meet-me

##### Attribute (CallNumMeetMeCode_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5619 |  | Alter answer number for meet-me

##### Attribute (CallNumMeetMeCode_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

#### MO(CallNumMeetMeCode_0)

5619 |  | Alter answer number for meet-me

Value: max. 4 digits (0-9,*,#)

Changes the directory number of this facility.

6501 |  | Directory name

Value: Printable character, length: 35

Changes the directory name of this facility.

5701 |  | BlockedFlag

Value: "true", "false"

#### MO(AlarmGroupMan)

5433 |  |

5533 |  |

5633 |  | Create Alarm group

##### Attribute (AlarmGroup_0)

to

##### Attribute (AlarmGroup_7)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

#### MO(AlarmGroup_0)

5633 |  | Create Alarm group

Value: max. 4 digits (0-9,*,#)

Changes the directory number of this facility.

6501 |  | Directory name

Value: Printable character, length: 35

Changes the directory name of this facility.

5701 |  | BlockedFlag

Value: "true", "false"

#### MO(PBXGroupMan)

5402 |  | Create PBX group

##### Attribute (PBXGroup_0)

to

##### Attribute (PBXGroup_15)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5502 |  | Delete PBX-group

##### Attribute (PBXGroup_0)

to

##### Attribute (PBXGroup_15)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5609 |  | Alter PBX group number

##### Attribute (PBXGroup_0)

to

##### Attribute (PBXGroup_15)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

#### MO(PBXGroup_0)

5609 |  | Alter PBX group number

Value: max. 4 digits (0-9,*,#)

Changes the directory number of this facility.

6501 |  | Directory name

Value: Printable character, length: 35

Changes the directory name of this facility.

5701 |  | BlockedFlag

Value: "true", "false"

3401 |  | Assigning members to a group

##### Attribute (3401_0)

to

##### Attribute (3401_19)

Value: Extension directory number

3501 |  | Hunt order

3502 |  | Exit position of PBX group

Value: max. 8 digits (0-9,*,#)

3503 |  | PBX queue announcement reference

Value range: "", "0" - "15"

3504 |  | PBX queue announcement delay

Value range: "6" - "15"

3505 |  | PBX queue overflow time

Value range: "0" - "255"

3506 |  | MOH source of PBX-group

Value range: "0" - "2"

3507 |  | Reroute on no answer

Value range: "0" - "255"

3508 |  | Flexible display

Value range: "0" - "2"

3509 |  | No Trunk Reroute

Value range: "0" - "1"

#### MO(ACDGroupMan)

5407 |  | Create ACD group

##### Attribute (ACDGroup_0)

to

##### Attribute (ACDGroup_7)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5507 |  | Delete ACD-group

##### Attribute (ACDGroup_0)

to

##### Attribute (ACDGroup_7)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5615 |  | Alter of ACD-group number

##### Attribute (ACDGroup_0)

to

##### Attribute (ACDGroup_7)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

#### MO(ACDGroup_0)

5615 |  | Alter of ACD-group number

Value: max. 4 digits (0-9,*,#)

Changes the directory number of this facility.

6501 |  | Directory name

Value: Printable character, length: 35

Changes the directory name of this facility.

5701 |  | BlockedFlag

Value: "true", "false"

3801 |  | ACD-group number

Value range: "", "0" - "8"

3802 |  | Time for 1st recorded answer

Value range: "0" - "255"

3803 |  | Time for 2nd recorded answer

Value range: "0" - "255"

3810 |  | Supervision time, T1, for statistics

Value range: "0" - "255"

3811 |  | Supervision time, T2, for statistics

Value range: "0" - "255"

3816 |  | Queue length

Value range: "1" - "63"

3817 |  | Dynamic queue

Value: "true", "false"

3818 Queue information to the caller

Value: "true", "false"

3819 |  | Time for passive marking

Value range: "0" - "255"

3820 |  | Postprocessing (clerical) time

Value range: "0" - "255"

3821 |  | Operator’s identity number for active

Value: "true", "false"

3822 |  | Call code after terminated call

Value: "true", "false"

3823 |  | Voice message to agent

Value: "true", "false"

3824 |  | Alternative answering position

Value: max. 4 digits (0-9,*,#)

3825 |  | Overflow time

Value range: "0" - "23"

3826 |  | Individual greeting

Value: "true", "false"

3827 |  | ACD night answer position

Value: max. 4 digits (0-9,*,#)

3828 |  | Enter multiple call code in clerical state allowed?

Value: "true", "false"

3829 |  | Number of timeouts before logout

Value range: "0" - "255"

3830 |  | End fix clerical time by pressing the clerical key before timeout

Value: "true", "false"

3901a |  | Voice answer 1 / Reference 0

3901b |  | Voice answer 1 / Reference 1

Value: "UUVV" UU=1,VV=1-32

0000 = no reference

3902a |  | Voice answer 2 / Reference 0

Value: "UUVV" UU=1,VV=1-32

0000 = no reference

3902b |  | Voice answer 2 / Reference 1

Value: "UUVV" UU=1,VV=1-32

0000 = no reference

3903a |  | ACD agent answer announcement / Reference 0

Value: "UUVV" UU=1,VV=1-32

0000 = no reference

3903b |  | ACD agent answer announcement / Reference 1

Value: "UUVV" UU=1,VV=1-32

0000 = no reference

3831 |  | Used Music on Hold source (for ACD)

#### MO(GroupCallPickupMan)

5405 |  | Create Call Pickup code

##### Attribute (GroupCallPickup_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5505 |  | Delete group call pick up code

##### Attribute (GroupCallPickup_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5614 |  | Alter group call pickup no.

##### Attribute (GroupCallPickup_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

#### MO(GroupCallPickup_0)

5614 |  | Alter group call pickup no.

Value: max. 4 digits (0-9,*,#)

Changes the directory number of this facility.

6501 |  | Directory name

Value: Printable character, length: 35

Changes the directory name of this facility.

5701 |  | BlockedFlag

Value: "true", "false"

4201 |  | State members in group

##### Attribute (4201_0)

to

##### Attribute (4201_319) Extension directory number

Note

The commands 5406 and 5506 do not exist on this level. The Call Pickup groups are not arranged as 16 different groups with 20 entries per group, but are handled as one large array of 319 entries.The entries 0-19 correspond with group 0. The entries 20-39 correspond with entries 0-19 of group 1. A group is created by setting at least one entry to a value other than "". A group is deleted by setting all entries to "".

#### MO(PrivateNetRouterMan)

5432 |  | Create Private Network Access Code

##### Attribute (PrivateNetRouter_0)

to

##### Attribute (PrivateNetRouter_999)

- Value: max. 4 digits (0-9,*,#)
- If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5532 |  | Delete Private Network Access Code

##### Attribute (PrivateNetRouter_0)

- to

##### Attribute (PrivateNetRouter_999)

- Value: max. 4 digits (0-9,*,#)
- If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5632 |  | Change of Private Network Access Code

##### Attribute (PrivateNetRouter_0)

- to

##### Attribute (PrivateNetRouter_999)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

#### MO(PrivateNetRouter_0)

5632 |  | Change of Private Network Access Code

Value: max. 4 digits (0-9,*,#)

Changes the directory number of this facility.

6501 |  | Directory name

Value: Printable character, length: 35

Changes the directory name of this facility.

5701 |  | BlockedFlag

Value: "true", "false"

9101 |  | Destination PBX
9101
Value | GUI
"0" | proprietary PBX
"1" | other vendor PBX

9102 |  | Call back allowed?

Value: "true", "false"

9103 |  | NPI for private calling/connected line identification
9103
Value | GUI
"16" | Private/Unknown(PNP/UNK)
"20" | Regionallevel0(PNP/RL0)
"18" | Regionallevel1(PNP/RL1)
"32" | Unknown/Unknown(UNP/UNK)

9104 |  | Call class
9104
Value | GUI
"" | Notspecified(nonIBERCOMcall)
"1" | interuserIBERCOMcall
"3" | intrauserIBERCOMcall

9105 |  | NPI for public calling/connected line identification

9110 |  | 1st-route choice

Trunk route directory number

9111 |  | NPI for private/public called number 1

9112 |  | Remove digits choice 1

Value range: "0" - "4"

9113 |  | Predigits choice 1

Value: max. 24 digits (0-9,*,#)

9114 |  | Travelling Class Mark 1

Value range: "0" - "7"

9115 |  | Complete called party NL 1

Value range: "", "1" - "32"

9116 |  | Subscriber called party NL 1

Value range: "", "1" - "20"

9117 |  | Node reference 1

Value range: "0" - "1000"

9120 |  | 2nd-route choice

Trunk route directory number

9121 |  | NPI for private/public called number 2

9122 |  | Remove digits choice 2

Value range: "0" - "4"

9123 |  | Predigits choice 2

Value: max. 24 digits (0-9,*,#)

9124 |  | Travelling Class Mark 2

Value range: "0" - "7"

9125 |  | Complete called party NL 2

Value range: "", "1" - "32"

9126 |  | Subscriber called party NL 2

Value range: "", "1" - "20"

9127 |  | Node reference 2

Value range: "0" - "1000"

9128 |  | Send expensive route warning tone 2

Value: "true", "false"

9130 |  | 3-rd route choice

Trunk route directory number

9131 |  | NPI for private/public called number 3

9132 |  | Remove digits choice 3

Value range: "0" - "4"

9133 |  | Predigits choice 3

Value: max. 24 digits (0-9,*,#)

9134 |  | Travelling Class Mark 3

Value range: "0" - "7"

9135 |  | Complete called party NL 3

Value range: "", "1" - "32"

9136 |  | Subscriber called party NL 3

Value range: "", "1" - "20"

9137 |  | Node reference 3

Value range: "0" - "1000"

9138 |  | Send expensive route warning tone 3

Value: "true", "false"

9140 |  | 4-th route choice

Trunk route directory number

9141 |  | NPI for private/public called number 4

9142 |  | Remove digits choice 4

Value range: "0" - "4"

9143 |  | Predigits choice 4

Value: max. 24 digits (0-9,*,#)

9144 |  | Travelling Class Mark 4

Value range: "0" - "7"

9145 |  | Complete called party NL 4

Value range: "", "1" - "32"

9146 |  | Subscriber called party NL 4

Value range: "", "1" - "20"

9147 |  | Node reference 4

Value range: "0" - "1000"

9148 |  | Send expensive route warning tone 4

Value: "true", "false"

#### MO(AutomatedAttendantGroupMan)

5424 |  | Create automated attendant

##### Attribute (AutomatedAttendant_0)

to

##### Attribute (AutomatedAttendant_31)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5524 |  | Delete automated attendant

##### Attribute (AutomatedAttendant_0)

to

##### Attribute (AutomatedAttendant_31)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5624 |  | Alter automated attendant

##### Attribute (AutomatedAttendant_0)

to

##### Attribute (AutomatedAttendant_31)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

#### MO(AutomatedAttendant_0)

5624 |  | Alter automated attendant

Value: max. 4 digits (0-9,*,#)

Changes the directory number of this facility.

6501 |  | Directory name

Value: Printable character, length: 35

Changes the directory name of this facility.

5701 |  | BlockedFlag

Value: "true", "false"

8701 |  | General-announcement reference

Value range: "", "1" - "42"

8702 |  | Error-announcement reference

Value range: "", "1" - "42"

8703 |  | Digit 0 related dir no

Value: max. 4 digits (0-9,*,#)

8704 |  | Digit 1 related dir no

Value: max. 4 digits (0-9,*,#)

8705 |  | Digit 2 related dir no

Value: max. 4 digits (0-9,*,#)

8706 |  | Digit 3 related dir no

Value: max. 4 digits (0-9,*,#)

8707 |  | Digit 4 related dir no

Value: max. 4 digits (0-9,*,#)

8708 |  | Digit 5 related dir no

Value: max. 4 digits (0-9,*,#)

8709 |  | Digit 6 related dir no

Value: max. 4 digits (0-9,*,#)

8710 |  | Digit 7 related dir no

Value: max. 4 digits (0-9,*,#)

8711 |  | Digit 8 related dir no

Value: max. 4 digits (0-9,*,#)

8712 |  | Digit 9 related dir no

Value: max. 4 digits (0-9,*,#)

8713 |  | Automated Attendant error reroute position

Value: max. 4 digits (0-9,*,#)

8714 |  | Waiting for full directory number

Value: "true", "false"

#### MO(CTIAutomatedAttendantMan)

5428 |  | Create CTI Group

##### Attribute (CTIAutomatedAttendant_0)

to

##### Attribute (CTIAutomatedAttendant_7)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5528 |  | Delete CTI Group

##### Attribute (CTIAutomatedAttendant_0)

to

##### Attribute (CTIAutomatedAttendant_7)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5628 |  | Alter CTI groups

##### Attribute (CTIAutomatedAttendant_0)

to

##### Attribute (CTIAutomatedAttendant_7)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

#### MO(CTIAutomatedAttendant_0)

5628 |  | Alter CTI groups

Value: max. 4 digits (0-9,*,#)

Changes the directory number of this facility.

6501 |  | Directory name

Value: Printable character, length: 35

Changes the directory name of this facility.

5701 |  | BlockedFlag

Value: "true", "false"

8730 |  | Greeting announcement reference

Value range: "", "1" - "24"

8731 |  | Instruction announcement reference

Value range: "", "1" - "24"

8732 |  | Error announcement reference

Value range: "", "1" - "24"

8733 |  | Default exit position

Value: max. 4 digits (0-9,*,#)

8734 |  | Use AA in combination with ACD group

Value: max. 4 digits (0-9,*,#)

#### MO(DISAwithPasswordMan)

5425 |  | Create DISA with password

##### Attribute (DISAwithPassword_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5525 |  | Delete DISA with password

##### Attribute (DISAwithPassword_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5625 |  | Alter DISA with password

##### Attribute (DISAwithPassword_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

#### MO(DISAwithPassword_0)

5625 |  | Alter DISA with password

Value: max. 4 digits (0-9,*,#)

Changes the directory number of this facility.

6501 |  | Directory name

Value: Printable character, length: 35

Changes the directory name of this facility.

5701 |  | BlockedFlag

Value: "true", "false"

8801 |  | DISA error reroute position

Value: max. 4 digits (0-9,*,#)

#### MO(MusicOnHoldMan)

5403 |  | Create music on hold

##### Attribute (MusicOnHold_0)

##### Attribute (MusicOnHold_1) (R12)

to

##### Attribute (MusicOnHold_7) (R12)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5503 |  | Delete music on hold channel

##### Attribute (MusicOnHold_0)

##### Attribute (MusicOnHold_1) (R12)

to

##### Attribute (MusicOnHold_7) (R12)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5610 |  | Alter music on hold number

##### Attribute (MusicOnHold_0)

##### Attribute (MusicOnHold_1) (R12)

to

##### Attribute (MusicOnHold_7)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

#### MO(MusicOnHold_0)

5610 |  | Alter music on hold number

Value: max. 4 digits (0-9,*,#)

Changes the directory number of this facility.

6501 |  | Directory name

Value: Printable character, length: 35

Changes the directory name of this facility.

5701 |  | BlockedFlag

Value: "true", "false"

3601 |  | Music source directory number

Value: Trunk directory number, D#00 (CPU port)

D420-D42F. D420-D42F is only allowed for Music on Hold, source 0. Each source may only be used for one Music source, including Background Music sources.

#### MO(BackgroundMusicMan)

5404 |  | Create background music

##### Attribute (BackgroundMusic_0)

to

##### Attribute (BackgroundMusic_2)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5504 |  | Delete background music channel

##### Attribute (BackgroundMusic_0)

to

##### Attribute (BackgroundMusic_2)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5611 |  | Alter background music number

##### Attribute (BackgroundMusic_0)

to

##### Attribute (BackgroundMusic_0)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

#### MO(BackgroundMusic_0)

5611 |  | Alter background music number

Value: max. 4 digits (0-9,*,#)

Changes the directory number of this facility.

6501 |  | Directory name

Value: Printable character, length: 35

Changes the directory name of this facility.

5701 |  | BlockedFlag

Value: "true", "false"

3601 |  | Music source directory number

Value: Trunk directory number, D#00 (CPU port). Each source may only be used for one Music source, including Music on Hold sources.

#### MO(VoiceAnswerReferenceMan)

5408 |  | Create voice answer

##### Attribute (VoiceAnswerReference_0)

to

##### Attribute (VoiceAnswerReference_15)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5508 |  | Delete voice answer

##### Attribute (VoiceAnswerReference_0)

to

##### Attribute (VoiceAnswerReference_15)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

5616 |  | Alter voice answer number

##### Attribute (VoiceAnswerReference_0)

to

##### Attribute (VoiceAnswerReference_15)

Value: max. 4 digits (0-9,*,#)

If this value is set to "" the facility is deleted. If this value is set to a free directory number, the facility is created or altered.

#### MO(VoiceAnswerReference_0)

5616 |  | Alter voice answer number

Value: max. 4 digits (0-9,*,#)

Changes the directory number of this facility.

6501 |  | Directory name

Value: Printable character, length: 35

Changes the directory name of this facility.

5701 |  | BlockedFlag

Value: "true", "false"

4701 |  | Reference number for voice answer

##### Attribute (4701_0) Voice answer reference 0

Value: "UUVVV"

UU = Announcement group

VVV = Announcement

##### Attribute (4701_1) Voice answer reference 1

Value: "UUVVV"

UU=Announcement group

VVV = Announcement

##### Attribute (4701_2) Voice answer reference 2

Value: "UUVVV"

UU=Announcement group

VVV = Announcement

Note

The range of UU depends on the BP release, the range of VVV depends on the BP release and the value of UU. Please see the BP documentation for details.

4702 |  | Voice answer storage

Value range: "", "0" - "63"

The slot of the card used for storage

#### MO(VoiceMemoryCardControlMan)

No commands/attributes

#### MO(CardS_I)

The MO name depends on the slot and individual of the voice card.

4601 |  | Record messages allowed ?

Value: "true", "false"

4602 |  | Record info allowed ?

Value: "true", "false"

4603 |  | Record announcements allowed ?

Value: "true", "false"

#### MO(IOPortMan)

No commands/attributes

#### MO(CardS_I)

The MO name depends on the slot and individual of the I/O Port.

6006 |  | Device type
6006
Value | GUI
"0" | 0: Printer
"1" | 1: O & M center with ECOM/ECEL
"2" | 2: Printer/terminal
"3" | 3: Printer xon/xoff type 1
"4" | 4: Printer xon/xoff type 2
"5" | 5: CIL without line protocol
"6" | 6: CIL with line protocol type 1
"7" | 7: Printer/terminal xon/xoff
"8" | 8: Hotel computer master
"9" | 9: Hotel computer slave
"10" | 10: Hotel computer, line protocol type 3
"11" | 11: O&M center with RASC and MS or CTI
"12" | 12: Hotel & CIL computer
"13" | 13: Hotel computer, line protocol type 4
"14" | 14: PC OperatorV1.x
"15" | 15: Common O&M interface for CSM

6007 |  | Character set
6007
Value | GUI
"0" | 0: PABX internal
"1" | 1: US-ASCII
"2" | 2: Swedish/Finnish ASCII
"3" | 3: IBM-PC compatible
"4" | 4: Danish/Norwegian ASCII

6009 |  | Baud rate

Value: The available Baud rates depend on the board type (CPU,IPU / Other) and the port type (IOU(V24) – SMU(Modem))

6009 CPU_D4, IPU – IOU (V24)
Value | GUI
"0" |
"6" | 300 Baud
"7" | 600 Baud
"8" | 1200 Baud
"9" | 1800 Baud
"10" | 2400 Baud
"11" | 3600 Baud
"12" | 4800 Baud
"13" | 7200 Baud
"14" | 9600 Baud
"16" | 19200 Baud

6009 CPU_D4, IPU – SMU (Modem)
Value | GUI
"0" |
"6" | 300 Baud
"7" | 600 Baud
"8" | 1200 Baud
"9" | 1800 Baud
"10" | 2400 Baud
"11" | 3600 Baud
"12" | 4800 Baud
"13" | 7200 Baud
"14" | 9600 Baud
"15" | 14400 Baud

6009 CPU_D, AUX, Other cards – IOU(V24)
Value | GUI
"0" |
"1" | 50 Baud
"2" | 75 Baud
"3" | 110 Baud
"4" | 135 Baud
"5" | 150 Baud
"6" | 300 Baud
"7" | 600 Baud
"8" | 1200 Baud
"9" | 1800 Baud
"10" | 2400 Baud
"12" | 4800 Baud
"13" | 7200 Baud
"14" | 9600 Baud

6009_NS
Value | GUI
"0" |
"7" | 600 Baud
"8" | 1200 Baud

6010 |  | Master/Slave

6011 |  | Autoselect allowed

Value: "true", "false"

6012 |  | Route on request
6012
Value | GUI
"0" |
"1" | O & M with RASC
"2" | ACD
"3" | CTI
"4" | CIL

6013 |  | Dial attempts

Value range: "0" - "5"

6014 |  | Dialled number

Value: max. 20 digits (0-9,*,#)

6015 |  | Dial pause (seconds)

Value range: "0" - "120"

6016 |  | Modem init string

Value: all printable characters, length:8

6017 |  | Mode selection for serial interface

This command is only available for port 1 of the CPU_D4 Board

6017
Value | GUI
"0" | RS232 (V24) interface active
"1" | RS485 interface active

#### MO(ScriptMgrMO)

No commands/attributes

Revision: B © Ericsson Enterprise 2005