BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2097
Show redirection number only?

The command is used to state whether the received redirection number shall de presented only. The number is used for display and other (CIL, MIS, CTI) purpose.

##### Valid data

Value | Meaning
Yes | only the redirection number is presented
No default | the redirection number and the A-number is presented

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005