BusinessPhone Communication Platform 7.0
Commands > Commands 6000...6999

## 6403
Format table

This command is used to determine the format of the data in the data record, so that it suits the connected external unit.

If data is sent to a connected external printer, a printer format needs to be selected. As a result a table header is obtained on the printout, which makes the information clearer.

If the format is changed for a channel that is marked faulty, it is possible that data are be lost.

#### FORMAT 00-29:
Data format for output to external unit.

00 No formatting, the channel is shut down |  |

01 Call data to computer according to MD110/standard format |  |

02 Call data to printer, with table header |  |

03 Call and hotel data to printer, with table header |  |

04 Call and hotel data to computer according to ASB150/ht format |  |

05 Call and hotel data to computer according to MD110/ht format |  |

06 Call and hotel data to computer according to HIS format |  |

07 Call and hotel data to computer according to CILHOTEL format |  |

08 Call and hotel data to computer according to CIL2HOTEL format |  |

09 Call and hotel data to computer according to CIL3HOTEL format |  |

10 Call and hotel data to computer according to CIL4HOTEL format |  |

11 Flexible CIL - format |  |

12-29 Reserve |  |

#### FORMAT 30-59:
Data format for input from external unit.

30 No formatting, the channel is shut down |  |

31-33 Reserve |  |

34 Hotel data according to ASB150/ht format |  |

35 Hotel data according to MD110/ht format |  |

36 Hotel data according to HIS format |  |

37 Hotel data according to CILHOTEL and CIL2HOTEL format |  |

38-59 Reserve |  |

#### FORMAT 60-99:
Data format for input from external unit.

60 No formatting, the channel is shut down |  |

61-63 Reserve |  |

64 Call and hotel data according to ASB150/ht format (bi-direct) |  |

65 Call and hotel data according to MD110/ht format (bi-direct) |  |

66 Call and hotel data according to HIS format (bi-direct) |  |

67 Call and hotel data according to CILHOTEL format (bi-direct) |  |

68 Call and hotel data according to CIL2HOTEL format (bi-direct) |  |

69 Call and hotel data according to CIL3HOTEL format (bi-direct) |  |

70 Call CTI (out) |  |

71 Call and hotel data according to CIL4HOTEL format (bi-direct) |  |

72 Flexible CIL - format |  |

73-99 Reserve |  |

#### Configuration of a bi-directional V.24 interface:

A bi-directional V.24 interface for CIL/HOTEL can only be installed on CIL-port 0 (command 6401 Initiate I/O ports). Activate the CIL-port 0 with YES (command 6402 Activate I/O ports?) and choose a format for bothway communication (64-99).

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005