BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1952
Signaling protocol

This command states the current ISDN-protocol to be used on the interface. It is possible to store various market-dependent ISDN protocols. The parameter defines selection of the current protocol to be used.

##### Valid data

- Australia
- ETSI
- Belgium
- Italy
- Netherlands
- Sweden
- Spain
- Finland
- Denmark
- New Zealand
- Swissnet

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005