BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2163
Signaling protocol

Defines the signalling protocol to be used towards the node defined by command 2164

##### Valid data

0 |  | None (default) |
1 - 100 |  | Reserved |
101 |  | ASB150 02 IP Gateway |
102 |  | H.323 Trunk Gateway |
103-255 |  | Reserved |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005