BusinessPhone Communication Platform 7.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 24 REROUTE

0 RER.NOTS |  | Not specified |
1 RER.TFR |  | Transfer |
2 RER.DNR |  | Diversion on no reply |
3 RER.BRK |  | Break in |
4 RER.CNF |  | Conference |
5 RER.OPR |  | Operator recall, after 'parked by operator' |
6 RER.NIN |  | Information not available, do not 'allow information' in the SEIZ |
7 RER.MG |  | Reroute call to MG |
8 RER.TFRBFA |  | Transfer before answer |
9 RER.CB |  | Callback |
10 RER.ACD |  | Reroute of ACD-call |
11 RER.SIL |  | Reroute on silent intrusion |
12 RER.BRKKEEP |  | Reroute, break in, keep display |
13 RER.LCRRDY |  | Least cost routing ready |
14 RER.LCRREQ |  | Least cost routing request |
15 RER.COBEXT |  | Reroute common bell extension |
16 RER.CANSWPOS |  | Exit storing and retrieving of messages |
17 RER.NMSG |  | Override multiple diversion to MG |
18 RER.FACEXIT |  | Exit from a facility to the desired directory number |
19 RER.CTI |  | Reroute caused by CTI |
20 RER.BYP |  | Reroute bypassing call diversion |
21 RER.DNA |  | Diversion on cordless not available |
22 RER.CNBYP |  | Reroute bypassing call diversion at calls to a CN party |
23 RER.CNDNR |  | Reroute on no reply to a CN diverted-to party |
24 RER.CNDIV |  | Reroute on CN call diversion immediate, on busy or on no reply when diverting party is another PBX |
25 RER.FACBUSY |  | Reroute from facility to exit position because the desired party is busy |
26 RER.CNDNA |  | Diversion on cordless not available to a CN diverted-to party |
27 RER.CONREC |  | Reroute on conversation recording |
28 RER.3PTYCONF |  | Reroute request to EX/OP from TR |
29 RER.OCN |  | Reroute on outcall notification |

Revision: F © Ericsson Enterprise 2005