BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1941
Explicit UUS service 1 activation request

This command states whether or not UUS (User-to-User Signalling) service 1 is requested explicitly at this interface.

##### Valid data

NO |  | not requested (implicitly) |
YES |  | explicitly requested |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005