BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2144
NPI aliases for called number - outgoing

The command “Number Plan Identifier (Number Plan and Type Of Number) aliases for called number - outgoing” is used for outgoing H.323 trunk calls. For each of the in command 2140 GK Primary NGK RAS transport address specified NGKs - Neighborhood GateKeeper - a list of up to 21 NPI aliases, for which the NGK can provide support to locate the corresponding GW - GateWay can be programmed. Each of them consists out of up to 12 digits and a corresponding type of number value.

##### Valid data per NGK

| Type of Number | Number information
1-21 | 00-10 | 0-12 digits
1-21 | 0 (default) | empty (default)

##### Valid data for Type of Number:

value | Number Plan | Type Of Number
00h (default) | Public | Unknown
01h | Public | International
02h | Public | National
03h | Public | Network specific
04h | Public | Subscriber
06h | Public | Abbreviated
08h | Private | Unknown
09h | Private | Regional level 2
0Ah | Private | Regional level 1
0Bh | Private | Network specific
0Ch | Private | Regional level 0 (local)
0Eh | Private | Abbreviated
10h | Unknown | Unknown

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005