BusinessPhone Communication Platform 7.0
Commands > Commands 7000...7999

## 7436
Active alarm attempts

This command determines the number of times alarm messages may be sent in situations where the receiving device does not respond. Value 0-5.

‘Active alarm’ is a function which transfers alarms to an external alarm receiver.

Commands 7420 Service area id, 7421 Identity of exchange and 7430 Active alarm on?-7437 Max active alarms per day concern active alarms.

Note

Value 0 means the string is not send via Modem, but used for direct connections via the CPU- or AUX- port.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2005