BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2199
H.323 Trunk GW Keep alive timer

Defines the length of the time interval between two availability check procedures towards a preconfigured gateway which is currently unavailable. Command 2199 H.323 Trunk GW Keep alive timer is used in case that there is no Gatekeeper. The timer is started as soon as a call to an IP gateway fails. In this situation BusinessPhone waits until the time out expires and then it calls automatically the “faulty” Gateway to see whether the called Gateway is still faulty or in operation again.

##### Valid data

1-65535 |  | seconds |
10 |  | default |

Note

It is not possible to deactivate this function

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005