BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2175
GK Time to live interval

On registration of a Trunk GW the GK forces the GW to activate its time to live mechanism with the herein specified timer value.

##### Valid data

0-255 |  | minutes |
0 |  | Time to live disabled |
10 |  | default |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005