BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1958
Common access number

This command states which of the dedicated route number(s) for this interface is the common access number.

##### Valid data

1-4 |  | digit numbers corresponding to route number |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005