BusinessPhone Communication Platform 7.0
Commands > Commands 4000...4999

## 4309
Keep answered call me

This command states how many answered “call me” messages can be saved. Thus, the size of the part of the E2 memory to be used for answered messages can be determined. This, of course, reduces the space for unanswered messages correspondingly.

Value 0 means that an unanswered message will be erased automatically upon answer. Except for a display telephone, where the message is erased via command. The range of values 1-99 specifies the number of answered messages saved. They can be accessed by a special procedure.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005