BusinessPhone Communication Platform 7.0
Commands > Commands 3000...3999

## 3508
Flexible display

This command defines the type of display layout, which will be used by the called PBX group members during ringing.

The flexible display will only be available on extensions, operators will not support this facility.

The display of the PBX group member will be updated to the regular extension display content after speech! The 2. row will contain the calling party and the 1. row in case of diversion the called party otherwise the PBX group independent of the PBX group settings for the display profile

1. display row | 2. display row | command 3508
PBX group | Calling party | Layout # 0
Called party | Calling party | Layout # 1
Called party | PBX group | Layout # 2

Only the 2. row is used by IP and cordless phones; some cordless phones, e.g. the DT 590 has both display rows.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005