BusinessPhone Communication Platform 7.0
Commands > Commands 3000...3999

## 3105
Name for Loudspeaker paging group 3

The command states which name text is to be shown on display telephones in the PABX with calls to a loudspeaker paging group.

##### Valid data

20 characters |  | (ACSII) |

Minimum required authority level from telephone: 3

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005