BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2077
First central answering position

The command is used to determine the 1st (of 3) central answer position for the system in a corporate network. The programmable numbers can either be,

1-8 CN reroute number when the answer position is located in other PBX. The programmed number must be the complete unique network number. |  |

1-4 Internal directory number when the answer position is located within the system. Tha call handling will be as for local rerouting, see further command 1104 Reroute position at night. |  |

Value ‘blank’, 1-8 digit number.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005