BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1014
Result tones to parent exchange?

The command is used to determine whether a result tone shall be sent to the parent exchange. This applies both to incoming and outgoing calls.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005