BusinessPhone Communication Platform 7.0
Warning Messages ASB 150 02 >

## 0xAB
Battery Backed-Up RAM Handler Error

Default definition: |  | ERROR |
Used by block: |  | OS |
Category: |  | DESIGNER |

An error occurred within the handler for the battery backed-up RAM.

- D1: Error code

- 01h: Given pool ID is invalid
- 02h: Not enough memory available.
- 03h: Given size of record is too large.
- 04h: Not an user of the given pool.
- 05h: Given map number is invalid.
- 06h: Record not found.
- 07h: Not enough memory for the free list available.
- 08h: Not a possible user of the given pool.
- 09h: Internal error within the battery backed-up RAM handler.
- 0Ah: Linked list not found.
- 0Dh: Memory error within the given map.
- 0Eh: Given map is not a data map.
- 0Fh: Given address is invalid.
- 10h: Given record is already linked.
- 11h: Given record is not linked.
- 14h: There is no user data.
- 15h: A pool withi the given pool ID already exists.
- 16h: Not being applied for a common pool.
- 17h: Not an owner of the given pool.
- 18h: Given pool has been resized less than expected.
- FFh: Pointer to record = FFh

- D2: Location (routine), where the error ooccurred.

- 0Bh: OS.BATPOOLCRE
- 0Ch: OS.BATPOOLRES
- 0Dh: OS.BATPOOLREM
- 0Eh: OS.BATPOOLADD
- 0Fh: OS.BATALLOC
- 10h: OS.BATALLINI
- 11h: OS.BATALLDNSM
- 12h: OS.BATALLINIDNSM
- 13h: OS.BATFREE
- 14h: OS.BATLFST
- 15h: OS.BATLLST
- 16h: OS.BATINS
- 17h: OS.BATINSBEF
- 18h: OS.BATUFST
- 19h: OS.BATUFSTFRE
- 1Ah: OS.BATUFSTFRERES
- 1Bh: OS.BATULST
- 1Ch: OS.BATULSTFRE
- 1Dh: OS.BATULNK
- 1Eh: OS.BATULNKFRE
- 1Fh: OS.BATULNKFRERES
- 20h: OS.BATFLST
- 21h: OS.BATFLSTDNSM
- 22h: OS.BATFNXT
- 23h: OS.BATFNXTDNSM
- 24h: OS.BATFPRV
- 25h: OS.BATFPRVDNSM
- 26h: OS.BATFNUM
- 27h: OS.BATFNUMDNSM
- 28h: OS.BATFIND
- 29h: OS.BATFINDDNSM
- 2Ah: OS.BATSEARCH
- 2Bh: OS.BATSEARCHDNSM
- 2Ch: OS.BATQLINKED

- D3: Undefined
- D4: Undefined

Revision: K © Ericsson Enterprise 2005