BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1915
Provision of calling line identification

The command is used to define whether calling ASB-party’s line directory number is allowed to be sent to network.

The following ASB-numbers to network parameters are available: NO: Calling ASB-party’s directory number not to network YES: Calling ASB-party’s directory number to network

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005