BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0190
Switch to non-IP network allowed ?

The command defines whether or not an extension is allowed to initiate a 'Switch over' of an ongoing call from the IP network to a circuit switched network.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005