BusinessPhone Communication Platform 7.0
Dialogs

## Backup Management

This dialog works as the backup management of the Gatekeeper’s registration table. The backup function prevents that all IP-Extensions are out of order after a system restart or a restart of the Gatekeeper’s IPU, as all the entries in the Gatekeeper’s registration table will be deleted.

### Backup enabled

You can enable the Gatekeeper backup by selecting the check box. If the backup function is enabled, a backup process will be started every 30 minutes. If the backup function is disabled, all IP-Extensions have to re-register themselves after a system or a board restart, in order to be active again.

### Immediate Backup

By pressing the Submit button the backup process will immediately create/update backup files on the Compact Flash card with the content of the current Gatekeeper‘s registration table, independent of whether the Backup function is enabled or disabled.

Note

Before removing the IPU board in case of service purposes, it is recommended to initiate an update of the backup files on the Compact Flash Card by pressing the Submit button in order to have the latest Gatekeeper‘s registration table status stored.

Revision: B © Ericsson Enterprise 2005