BusinessPhone Communication Platform 7.0
Commands > Commands 3000...3999

## 3802
Time for 1st recorded answer

Recorded announcements can be supplied for calls to an ACD-group. Two recorded announcements can be programmed for ACD. This command is used to state the time to elapse before the 1st recorded announcement.

Range of values = 0-255 s

If the time is set to 0, no recorded announcement will be sent.

See command 3901 First voice answer which states the reference numbers for the first voice answer.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005