BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1938
Connect message at inband information available

#### New command - since release 14 R4A:

Defines if a CONNECT message shall be sent, at non-direct transit calls and inband information is available to the originating network (e.g. calls to a mobile extension, external diverted/rerouted calls).

This gives the caller the possibility to hear tones or announcements provided by the terminating party after the complete called party number is sent

##### Valid data

16 | CONNECT at PROGRESS message with inband info
32 | CONNECT at PROCEED message with inband info
64 | CONNECT at ALERTING with inband info
112 | default (all 3 possibilities are enabled)

Note

The value is needed for script programming

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005