BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2087
Transit counter

The command defines the maximum amount of allowed transit call setups to prevent uncontrolled loops in the network.

##### Valid data

1 |  | (default) |
2-31 |  |  |

Default Value = 7

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005