BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2191
H.323 Trunk GW Primary GK IP-address

Defines the IP-address of the Gatekeeper to which the H.323 Trunk Gateway has to register

##### Valid data

0.0.0.0 - 255.255.255.255:(0 - 65535) |  |  |
0.0.0.0 (default) |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005