BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1943
UU-information in ALERT message

This command states whether or not it is allowed to include UUI (User-to-User Information) in the ALERTING message at this interface.

##### Valid data

No |  | (not allowed) |
Yes |  | allowed |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005