BusinessPhone Communication Platform 7.0
Commands > Commands 7000...7999

## 7435
Active alarm pause

This command determines the number of seconds after which an unsuccessful attempt to send an alarm is to be repeated. Value 0-120 seconds.

‘Active alarm’ is a function which transfers alarms to an external alarm receiver.

Commands 7420 Service area id, 7421 Identity of exchange and 7430 Active alarm on?-7437 Max active alarms per day concern active alarms.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2005