BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2162
Port number

This command defines the TCP “entry” port associated with the feature and/or protocol

##### Valid data

0-1024 |  | reserved |
1025--6000 |  |  |
1718 |  | reserved for multicast, not used in ASB 150 02 R14 |
1719 |  | H.323 Trunk GW Primary GK RAS port number |
1720 |  | H.323 Extension GW Q.931 port |
6000 |  | I/O port 1 |
6001 |  | I/O port 2 |
6002 |  | I/O port 3 |
6003 |  | I/O port 4 |
6005-6999 |  |  |
7000 |  | ASB 150 02 IP gateway |
7001-65535 |  |  |
8100 |  | reserved by command 2157 |
9000 |  | reserved by IP trace function |
10000 |  | reserved |
10010 |  | reserved by H.323 Extension GW RAS-port |
10030 |  | reserved by H.323 Trunk GW RAS-port |
10040 |  | reserved by H.323 Trunk GW Q.931-port |
30000 |  | reserved |

Note

The table is already predefined with port numbers to each available application. So far, there is no need to modify the table.
If you change the port of the ASB 150 02 IP gateway to another value, please take care that the new port number is included in the PNR tables (command 2164) off all the other network nodes which are referring to this system.The port number defined in command 2164 must always be equal with the port number defined in the destination node.
Further take care that the defined port numbers are not in conflict with the port numbers defined by command 2157.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005