BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1035
Travelling class mark (TCM)

This command defines the ‘Travelling Class Mark (TCM)’ for the incoming trunk. If no ‘Travelling Class Mark (TCM)’ is received from preceding node the defined TCM-value is used to decide if call can continue as transit network call. If the defined TCM-value is lower than any of the TCM-values, assigned to the network routes (see commands 9114 Travelling Class Mark 1, 9124 Travelling Class Mark 2, 9144 Travelling Class Mark 4), the call setup to the network is not allowed. Value = (0-7) Default value = 7

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005