BusinessPhone Communication Platform 7.0
Commands > Commands 4000...4999

## 4102
Operator answer reference

This command states the reference number for voice answer.

The reference number is entered as: uuvv

where

uu = 01 (always) |  |

vv = 01-32 (see command 4401 Voice Announcements) |  |

uuvv = blank (no voice answer) |  |

It is required that the stated reference (uuvv) has been recorded with a system telephone in accordance with command 4401 Voice Announcements.

When the operator answers a new incoming external call, a voice answer in accordance with a stated reference is supplied. After the voice answer has been supplied the operator has speech connection with the caller.

It is required that the stated reference (uuvv) has been recorded with a system telephone in accordance with command 4401 Voice Announcements.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005