BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0172
Fixed diversion destination for internal calls, if cordless/IP-Instrument is not available

This command is used to activate diversion on not available for internal calls. Diversion on not available could be a result of a not attainable cordless phone or a not registered IP-Instrument.

If no diversion address is specified, the diversion is inactive.

Note

After a call diversion “on not available”, no repeated call diversion is possible any more.

##### Valid data

1 |  | directory number |
2-8 |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005