BusinessPhone Communication Platform 7.0
Facility Description – General

## Feature Codes

The following table includes all feature codes accessable via the telephone in ASB 150 02:

Code | Feature

*0# | internal directory book
#0* | external directory book
* 0 0 * | individual programming
* 0 0 # | programming (individual and system)
* 2 1 # | diversion direct - activate
# 2 1 # | diversion direct - deactivate
* 2 2 * | individual external diversion - activate
* 2 2 * # | individual external diversion - reactivate
# 2 2 # | individual external diversion - deactivate
* 2 3 * | information - activate
# 2 3 # | information - deactivate
* 2 8 # | Tandem function / PBX Group - Logon
# 2 8 # | Tandem function / PBX Group - Logoff slave
* 2 8 * * # | All PBX Group - Logon
# 2 8 * * # | All PBX Group - Logoff slave
* 3 1 # | Hotel - check in, check out, room status
* 3 2 # | Hotel - administrative wake up
* 3 2 * | Reminder - activate
# 3 2 # | Reminder - deactivate
* 3 3 * | Hotel - Guest room clean
* 3 4 # | Hotel - blocking of RTR and DID
* 3 9 # | ISDN - Malicious Call Identification
* 4 0 # | ACD - print procedure
* 4 1 # | Call Metering - activation / deactivation of cost indication
* 4 5 # | Call Metering - own accumulated costs
* 4 6 # | Call Metering - cost of last call
* 4 8 # | ISDN - Caller List
* 5 1 * | programm abbreviated number dialling - individual numbers
# 5 1 # | delete abbreviated number dialling - individual numbers
* 5 3 # | Alarm - activation
* 5 4 # | Alarm - deactivation
* 5 5 * | Hotel - wake up order / cancel
* 5 8 # | Dictaphone function
* 5 9 # | Message system
* 6 0 * | Bypass call diversion and IP-calls
* 6 1* | IPU LAN over second route access
* 6 5 * | ACD - silent intrusion
* 7 2 # | Authority - activate
# 7 2 * | Authority - deactivate
* 7 2 * | Authority - temp. bypass blocked ext.
# * 7 2 | Authority - change password
* 7 3 # | Common Bell - pick-up code
* 7 9 # | Alarm - read out
* 8 # | Night switching - activate / deactivate system
* 8 0 # | Night switching - activate / deactivate, all trunk groups
* 8 1 # | Night switching - activate / deactivate, trunk group 1
* 8 2 # | Night switching - activate / deactivate, trunk group 2
* 8 3 # | Night switching - activate / deactivate, trunk group 3
* 8 4 # | Night switching - activate / deactivate, trunk group 4
* 8 5 # | Night switching - activate / deactivate, trunk group 5
* 8 6 # | Night switching - activate / deactivate, trunk group 6
* 8 7 # | Night switching - activate / deactivate, trunk group 7
* 8 8 # | Night switching - activate / deactivate, trunk group 8
* 8 9 0 | Night switching - activate / deactivate, ACD group 1
* 8 9 1 | Night switching - activate / deactivate, ACD group 2
* 8 9 2 | Night switching - activate / deactivate, ACD group 3
* 8 9 3 | Night switching - activate / deactivate, ACD group 4
* 8 9 4 | Night switching - activate / deactivate, ACD group 5
* 8 9 5 | Night switching - activate / deactivate, ACD group 6
* 8 9 6 | Night switching - activate / deactivate, ACD group 7
* 8 9 7 | Night switching - activate / deactivate, ACD group 8
* 8 9 8 | Night switching - activate / deactivate, all ACD groups
* 9 * | Account codes
* 9 0 # | Maintenance - Instrument test
* 9 1 # | Maintenance - Alarm
* 9 2 * | External voice mail - activate
# 9 2 * | Extenal voice mail - deactivate
* 9 3 # | Maintenance - number of open / restricted trunk accesses
* * * | Last extenal number redial
* * 0 - * * 9 | activate Abbreviated number dialling - individual numbers

Revision: E © Ericsson Enterprise 2005