BusinessPhone Communication Platform 7.0
Facility Description – General

## Introduction

### Overview

This document, together with a number of subdocuments, describes all functions in ASB 150 02.

#### Facilities

Each subdocument, xxx/155 34-ASB 150 02 Uen etc., describes the facilities in alphabetical order.

#### Definition

A concise description of the facility is provided under this heading.

#### Use

Under this heading is stated in which way the user can utilise the facility.

#### Operation

Under this heading is described how the facility is operated from the following current telephones types:

- Analog Telephone, Dialog 4106, 4147 and 4186
- Dialog 4220 Lite, DBC 220
- Dialog 4222 Office, DBC 222
- Dialog 4223 Professional, DBC 223

If operation is different for the various telephones the procedures will be described under different subheadings.

The Dialog 4224 Operator, DBC 224, is described seperately in the Facility Description Operator (380/155 34-ASB 150 02 Uen).

Note

For operation of older telephones mentioned under Telephones delivered in previous releases of ASB 150 02 in this document, see the User’s Guide for the individual telephone type.

#### Capacity

Capacity restrictions (if any) for the facility are described under this heading.

For example it is possible to state here the number of groups for a certain function or the maximum number of extensions that can be members of a certain group.

#### Limitations

Under this heading is stated whether the facility has functional limitations, for example whether it is non applicable with regard to certain traffic cases.

#### Programming

Here are the programming commands stated that must be executed to access the facility.

The programming commands are to be executed in the sequence stated.

Each command is presented with a header and command number in accordance with the following pattern:

0301 |  | Key function

After the command number has been entered the display shows an image with the following pattern:

The second row shows, from the left:

- Explanatory text for the command
- Command number (0301)
- Fields to be completed in accordance with command description (xxxx, y, zz)

The programming procedures are described in section System Programming.

Certain functions, for example the function of the telephone's keys, can be programmed by the user. This is called and described in section Individual Programming.

Note

Programming from other types of system telephones may show a little different layouts depending upon the display type.

For detailed information see section System Programming.

#### Equipment

Under this heading is stated whether any special printed board assembly or other hardware needs to be connected in order to access the facility.

### General

The “Facility Description” describes all facilities in ASB 150 02.

Each facility is described in accordance with a common pattern with the same headings used in all descriptions.

The documents also embrace the description of common functions and types of telephone.

Revision: E © Ericsson Enterprise 2005