BusinessPhone Communication Platform 7.0
Warning Messages ASB 150 02 >

## 0x0D
Digital Link Error

Default definition: |  | UNDEFINED |
Default limit: |  | 65000 |
Used by block: |  | LS |
Category: |  | DESIGNER |

This warning indicates a new alarm condition on the international / national bits, or a new alarm condition for layer 2 on the current digital link.

- D1: Alarm condition

- 01h: Alarm condition on the international/national bits
- 02h: Alarm condition on layer 2.

- D2: Card position
- D3: Undefined
- D4: Undefined

Revision: K © Ericsson Enterprise 2005