BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2270
Assign A-number of Mobile Extensions

This command is used to assign A-numbers of Mobile Extensions to their internal directory numbers.

##### Valid data

| internal directory Number | A-Number
1-100 |  | 0-20 digits (0 to 9)
1-100 | empty (default) | empty (default)

Note

The A‑number has to be entered as it should be dialled - after route access (including leading zeros - after route seizure).

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005