BusinessPhone Communication Platform 7.0
Commands > Commands 4000...4999

## 4602
Record info allowed ?

Voice messages, voice information and voice answers are stored on “voice memory boards”, VMU.

This command determines whether voice information may be recorded on the stated board.

##### Valid data

Yes |  |  |
No |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005