BusinessPhone Communication Platform 7.0
Warning Messages ASB 150 02 >

## 0x16
Buffer Usage Error

Default definition: |  | ERROR + TRIG |
Used by block: |  | OS |
Category: |  | DESIGNER |

The OS.BUFFER macro has been used in an invalid way.

- D1: BUFFLOG from buffer (last executed operation).

- 00h: Linked buffer, last in the chain.
- 01h-EFh: Linked buffer, next buffer forward.
- F0h: Released buffer.
- F1h: Job buffer, OS own (buffer 0).
- F2h: Job buffer, common.
- F3h: Keep marked buffer.
- F4h: Requested buffer.
- F5h: Unlinked buffer.
- F6h-FFh: Not valid, spare for future use.

- D2: BUFFJID from buffer (job identity).

- 40h-FBh: OS-logged jobsignal type (ST, job enter)
- FEh: Buffer is handled during init.
- FFh: OS-handled buffer (job exit)

- D3: Undefined
- D4: Undefined

Revision: K © Ericsson Enterprise 2005