BusinessPhone Communication Platform 7.0
Facilities

## Clock And Diary

## Definition

The system contains a realtime clock that is used to state the time and date of various functions in the system.

## Use

The clock in the system is used for the following functions:

- Reading of time and date on telephones with display
- To state time for CIL-(Call Information Logging) function
- Wake up in hotel system
- To block room-to-room traffic in hotel system at preprogrammed times
- For reminder facility, that is to call extension at programmed time
- Stamp sent messages with time and date that can be read off later
- Stamp alarms in the alarm centre function

In conjunction with an ISDN network, the clock of the ASB 150 02 system can be synchronised against the clock provided by the ISDN network.

## Operation

### DBC 222, DBC 212, DBC 631, DBC 223, DBC 213 and DBC 662 Telephones

Date and time are shown on the top row of the DBC 222, DBC 212, DBC 631, DBC 223, DBC 213 and DBC 662 telephones’ display.

The time can be displayed in the 24- or 12-hour mode.

#### 24 hour mode

The display shows e.g.:

#### 12 hour mode

The display shows e.g.:

## Capacity

The time can be displayed in both the 24- and 12-hour modes. The diary takes into consideration the different number of days per month as well as leap years.

## Limitations

The clock has battery backup and can withstand loss of power for up to 200 hours.

## Programming

### Programming via the Telephone

6101 |  | Set year month day

Enter:

YY |  | year |  | (00-99) |
MM |  | month |  | (01-12) |
DD |  | day |  | (01-31) |

6103 |  | Set hour minute second

Enter:

HH |  | hour |  | (00-23) |
MM |  | minute |  | (00-59) |
SS |  | second |  | (00-59) |

6104 |  | 12h mode, display

For 12-hour mode the time is stated with AM and PM.

Default data: N = 24-hour mode.

### Programming via BMS

Time and date of ASB 150 02 can be set via BMS.

The command “set clock” is stated in the menu “system/system parameter”.

For the time syncronisation with the ISDN network set following command in addition

2066 |  | ISDN Link for Automatic Time Adjustment

## Equipment

None

Revision: D © Ericsson Enterprise 2005