BusinessPhone Communication Platform 7.0
Commands > Commands 5000...5999

## 5511
Delete call number for alternative paging

ASB 150 permits connection of external equipment for paging via radio or a magnetic loop. Connection takes place via a trunk (external line) board that has been reserved for this purpose.

This command is used to delete the call number for alternative paging.

Alternative paging means that the pager himself/herself can control the paging receiver by stating a mode digit, sending a message or supplying a spoken message.

Commands 5510 Delete call number for standard paging and 5512 Delete answer number for meet-me are used to delete other directory numbers (if any) that have been created for paging.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005