BusinessPhone Communication Platform 7.0
Commands > Commands 6000...6999

## 6431
Test protocol port address

This command can be used to define the board number and the individual of the test protocol IO port, where data transfer should be handled.

The value “pp” defines the board number, where the test protocol port is located.

The value “iii” includes the individual number of the test protocol port on the board.

Note

The desired port can only be entered, if the Device Type (command 6006 Device type) for this port is already set to value 14!

Minimum required authority level from telephone: YES

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005