BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1033
Impedance adaption for transit calls

The command is used to state whether or not the automatic trunk impedance adaption (ATIA) has to be used during transit calls. The parameter programmed by this command is relevant only if ATIA is activated by superior command 1032 Trunk impedance adaption.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005