BusinessPhone Communication Platform 7.0
Commands > Commands 3000...3999

## 3810
Supervision time, T1, for statistics

Time T1 is a time that is initiated in a call to an ACD-operator. The number of calls answered before and after the time T1 is registered. This command is used to alter the supervision time T1 for ACD-statistics. Range of values 1-255 seconds.

See commands 3812 Number of answered calls before time T1 and 3813 Number of answered calls after time T1.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005