BusinessPhone Communication Platform 7.0
Warning Messages ASB 150 02 >

## 0xC1
Switch Channel Release Error

Default definition: |  | ERROR + TRIG |
Used by block: |  | SX |
Category: |  | DESIGNER |

The SX-block has detected, that an RP is still connected to a PCM channel although this channel has been released and delivered to a new party by OU.CHANNEL calls.

- D1: Type of error

- Bit 0 ... Listening connection
  0 ... No error
  1 ... When a PCM-channel is requested, there is still one RP listening to this channel.
- Bit 1 ... Sending connection
  0 ... No error
  1 ... When a PCM-channel is requested, there is still one RP sending on this channel.
- Bit 2 ... Speech connection
  0 ... No error
  1 ... When a PCM-channel is requested, the previously connected RP is still in 'speech connection' (forgotten TRANSM, TRMCONNOM or TRANSM,TRMCONSPK).
- Bit 3 ... Not used
- Bit 4 ... Not used
- Bit 5 ... Not used
- Bit 6 ... PCM-bus
- Bit 7 ... Not used

- D2: Card position, which is incompletely disconnected from a PCM-channel.
- D3: Card position, which should be connected to the PCM-channel.
- D4: Individual number, which should be connected to the PCM-channel.

Revision: K © Ericsson Enterprise 2005