BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2186
Network Node reference

The commands 2186 Network Node reference and 2187 Network Node Password together with 2163 Signaling protocol and 2164 Network IP address form the layout of the Network Node Table as it is valid with ASB 150 02 R14.

##### Valid data

0-1000 |
empty (default) |

Example:

The Network Node Table (also called IP Reference table or ’1000’ node table) shows all known Gateways

Network Node reference | Signalling protocoll | Network IP address | Network Node Password
1 | 102 | 10.155.166.177:10040 |
2 | 102 | 10.133.144.155:10040 |
2 | 102 | 10.133.144.156:10040 |
3 | 102 | 10.188.199.122:10040 | IP400_01

Note

Command 2186 Network Node reference represents the nodes. As shown in the table above one of command 2186 Network Node reference (here 2) can have several entries, which means that node 2 has two IPUs. In this case the originating IPU (of node 1) searches for all valid entries in the Network Node Table, which reduces the PNR - configuration effort.

Note

If BusinessPhone makes an outgoing call then the call signalling Port number (Q.931) (part of command 2164 Network IP address) of the IP Reference table must correspond with the Q.931 - Port number of the destination PBX. In case, that the destination PBX is a BusinessPhone, then the Port number has to correspond with the value of command 2194 H.323 Trunk GW Q.931‑port of the destination BusinessPhone.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005