BusinessPhone Communication Platform 7.0
Commands > Commands 4000...4999

## 4603
Record announcements allowed?

It is possible to determine whether or not a certain VMU board may be used for voice announcements.

##### Valid data

Yes |  |  |
No |  | (default) NO = Voice announcement can not be stored on board |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005