BusinessPhone Communication Platform 7.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 64 BTCSIGNAL

01h BTSDETEPTS |  | 'Proceed to send' detected |
03h BTSBANSWER |  | B-answer |
04h BTSLINEOK |  | Trunk line OK |
05h BTSLINFAUL |  | Trunk line faulty |
06h BTSEOS |  | 'End of selection' detected |
07h BTSDIGIT |  | Digit received |
08h BTSINCCALL |  | Incoming call |
09h BTSINCDID |  | Indialling call |
0Ah BTSINCIOP |  | Incoming call with internat. operator |
0Bh BTSINCRING |  | Incoming call with external ring signal |
0Ch BTSDETEPES |  | Periodic end signal detected |
0Dh BTSINQUIRY |  | Inquiry signal detected |
0Eh BTSDISCONN |  | Disc. or time out at incoming ring |
0Fh BTSFREE |  | Trunk is free |
10h BTSPAGING |  | Paging in progress |
11h BTSPAGABS |  | Paging equipment absent |
12h BTSBLOCKED |  | Trunk line blocked |
13h BTSDEBLOCK |  | Trunk line deblocked |
14h BTSEOSFREE |  | EOS detected, subscriber free |
15h BTSEOSBUSY |  | EOS detected, subscriber busy |

Revision: F © Ericsson Enterprise 2005